<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="96.5" x2="0" y2="3.5" width="0" layer="20"/>
<wire x1="0" y1="3.5" x2="3.5" y2="0" width="0" layer="20" curve="90"/>
<wire x1="3.5" y1="0" x2="96.5" y2="0" width="0" layer="20"/>
<wire x1="96.5" y1="0" x2="100" y2="3.5" width="0" layer="20" curve="90"/>
<wire x1="100" y1="3.5" x2="100" y2="96.5" width="0" layer="20"/>
<wire x1="100" y1="96.5" x2="96.5" y2="100" width="0" layer="20" curve="90"/>
<wire x1="96.5" y1="100" x2="3.5" y2="100" width="0" layer="20"/>
<wire x1="3.5" y1="100" x2="0" y2="96.5" width="0" layer="20" curve="90"/>
<text>CHA/V-ES basado en jonasbers.com/chav/</text>
<text>pcb by luix github.com/Ttreintaysiete/chaves</text>
<text>version 3</text>
<text>H</text>
<text>G</text>
<text>V</text>
<text>H</text>
<text>G</text>
<text>V</text>
<text>H</text>
<text>G</text>
<text>V</text>
<text>H</text>
<text>G</text>
<text>V</text>
<text>H</text>
<text>G</text>
<text>V</text>
<text>H</text>
<text>G</text>
<text>V</text>
<text>VCO1</text>
<text>VCO2</text>
<text>VCO3</text>
<text>VCO4</text>
<text>VCO5</text>
<text>VCO6</text>
<text>BLUE</text>
<text>GREEN</text>
<text>RED</text>
<text>L</text>
<text>*</text>
<text>O</text>
<text>P</text>
<text>Cha-Cha-CHAV!!</text>
<text>VCO1</text>
<text>VCO2</text>
<text>VCO3</text>
<text>VCO6</text>
<text>VCO5</text>
<text>VCO4</text>
<text>L</text>
<text>*</text>
<text>O</text>
<text>P</text>
<text>R</text>
<text>G</text>
<text>B</text>
</plain>
<libraries>
<library name="40xx">
<description>&lt;b&gt;CMOS Logic Devices, 4000 Series&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola &lt;i&gt;CMOS LOGIC DATA&lt;/i&gt;; book, 02/88, DL131 REV 1
&lt;li&gt;http://www.elexp.com
&lt;li&gt;http://www.intersil.com
&lt;li&gt;http://www.ls3c.com.tw/product/1/COMOS.html
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL14">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="MusicThingModular">
<description>&lt;B&gt;Music Thing Modular parts library &lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;Components for Eurorack modular synths 
&lt;/ul&gt;</description>
<packages>
<package name="M9040P">
<description>Toggle Switch T-80-T from Rapid</description>
</package>
<package name="TO92-ECB">
<description>&lt;b&gt;TO-92&lt;/b&gt; Pads In Line E C B from top&lt;p&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="C050-025X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 2.5 x 7.5 mm</description>
</package>
<package name="0204V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 2.5 mm</description>
</package>
<package name="1X01">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="LED5MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
5 mm, round</description>
</package>
<package name="1X12-CB">
</package>
<package name="1X09-BIG">
</package>
<package name="DCJACK_2MM_PTH">
<description>DJ Jack 2.0mm PTH Right-Angle</description>
</package>
</packages>
</library>
<library name="pot-alps">
<packages>
<package name="ALPS_POT_VERTICAL">
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="2X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X04">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="holes">
<description>&lt;b&gt;Mounting Holes and Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="3,0">
<description>&lt;b&gt;MOUNTING HOLE&lt;/b&gt; 3.0 mm with drill center</description>
</package>
</packages>
</library>
<library name="special-drill">
<description>&lt;b&gt;Special drills&lt;/b&gt;&lt;p&gt;
For drills bigger as 0.51602 Inch you must draw a circle in Layer 20 Dimension.&lt;br&gt;
See also HELP HOLE,</description>
<packages>
<package name="DRILL_0.1875">
<description>&lt;b&gt;3/16" Marker&lt;/b&gt; 187.5 thousands of an inch</description>
</package>
</packages>
</library>
<library name="pj302m">
<packages>
<package name="PJ302M">
<description>Library part for the PJ302M horizontal / right angled mount 3.5 mm jack socket available from Thonk.co.uk among others.</description>
</package>
</packages>
</library>
<library name="diode">
<packages>
<package name="DO41-10">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 2.54 mm, horizontal, grid 10.16 mm</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="40xx" package="DIL14" value="40106N">
<attribute name="VALUE"/>
</element>
<element name="C1" library="adafruit" package="C050-025X075" value="101">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="adafruit" package="C050-025X075" value="102">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="POT1" library="pot-alps" package="ALPS_POT_VERTICAL" value="10k"/>
<element name="C4" library="adafruit" package="C050-025X075" value="101">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="adafruit" package="C050-025X075" value="102">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="adafruit" package="C050-025X075" value="103">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="adafruit" package="C050-025X075" value="104">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="adafruit" package="C050-025X075" value="103">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="adafruit" package="C050-025X075" value="104">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="adafruit" package="C050-025X075" value="101">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="adafruit" package="C050-025X075" value="104">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="adafruit" package="C050-025X075" value="101">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="adafruit" package="C050-025X075" value="104">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="POT2" library="pot-alps" package="ALPS_POT_VERTICAL" value="10k"/>
<element name="POT3" library="pot-alps" package="ALPS_POT_VERTICAL" value="10k"/>
<element name="POT4" library="pot-alps" package="ALPS_POT_VERTICAL" value="10k"/>
<element name="POT5" library="pot-alps" package="ALPS_POT_VERTICAL" value="10k"/>
<element name="LDR1" library="adafruit" package="0204V" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RJ" library="adafruit" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="GJ" library="adafruit" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BJ" library="adafruit" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="adafruit" package="C050-025X075" value="103">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C20" library="adafruit" package="C050-025X075" value="104">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="adafruit" package="C050-025X075" value="103">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="adafruit" package="C050-025X075" value="104">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C16" library="adafruit" package="C050-025X075" value="103">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C17" library="adafruit" package="C050-025X075" value="104">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C18" library="adafruit" package="C050-025X075" value="103">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C21" library="adafruit" package="C050-025X075" value="104">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C22" library="adafruit" package="C050-025X075" value="103">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C23" library="adafruit" package="C050-025X075" value="104">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C24" library="adafruit" package="C050-025X075" value="103">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C25" library="adafruit" package="C050-025X075" value="104">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JGND" library="adafruit" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="+5V" library="adafruit" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JHSYNC" library="adafruit" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JVSYNC" library="adafruit" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="E$5" library="holes" package="3,0" value=""/>
<element name="E$6" library="holes" package="3,0" value=""/>
<element name="E$7" library="holes" package="3,0" value=""/>
<element name="E$8" library="holes" package="3,0" value=""/>
<element name="JP8" library="pinhead" package="2X03" value="">
<attribute name="VALUE"/>
</element>
<element name="JP3" library="pinhead" package="2X03" value="">
<attribute name="VALUE"/>
</element>
<element name="JP9" library="pinhead" package="2X03" value="">
<attribute name="VALUE"/>
</element>
<element name="JP10" library="pinhead" package="2X03" value="">
<attribute name="VALUE"/>
</element>
<element name="JP11" library="pinhead" package="2X03" value="">
<attribute name="VALUE"/>
</element>
<element name="JP12" library="pinhead" package="2X03" value="">
<attribute name="VALUE"/>
</element>
<element name="R1" library="adafruit" package="0204V" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="adafruit" package="0204V" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="adafruit" package="0204V" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="adafruit" package="0204V" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP13" library="pinhead" package="1X04" value="">
<attribute name="VALUE"/>
</element>
<element name="U$1" library="MusicThingModular" package="M9040P" value="T-80-T-SPDT-ON-OFF-ON"/>
<element name="U$2" library="MusicThingModular" package="M9040P" value="T-80-T-SPDT-ON-OFF-ON"/>
<element name="U$3" library="MusicThingModular" package="M9040P" value="T-80-T-SPDT-ON-OFF-ON"/>
<element name="U$4" library="MusicThingModular" package="M9040P" value="T-80-T-SPDT-ON-OFF-ON"/>
<element name="U$5" library="MusicThingModular" package="M9040P" value="T-80-T-SPDT-ON-OFF-ON"/>
<element name="U$6" library="MusicThingModular" package="M9040P" value="T-80-T-SPDT-ON-OFF-ON"/>
<element name="U$7" library="MusicThingModular" package="M9040P" value="T-80-T-SPDT-ON-OFF-ON"/>
<element name="U$8" library="MusicThingModular" package="M9040P" value="T-80-T-SPDT-ON-OFF-ON"/>
<element name="U$9" library="MusicThingModular" package="M9040P" value="T-80-T-SPDT-ON-OFF-ON"/>
<element name="U$10" library="MusicThingModular" package="M9040P" value="T-80-T-SPDT-ON-OFF-ON"/>
<element name="U$11" library="MusicThingModular" package="M9040P" value="T-80-T-SPDT-ON-OFF-ON"/>
<element name="U$12" library="MusicThingModular" package="M9040P" value="T-80-T-SPDT-ON-OFF-ON"/>
<element name="R5" library="adafruit" package="0204V" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="adafruit" package="0204V" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="adafruit" package="0204V" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="T1" library="MusicThingModular" package="TO92-ECB" value="bc547">
<attribute name="VALUE"/>
</element>
<element name="LED1" library="adafruit" package="LED5MM" value="">
<attribute name="VALUE"/>
</element>
<element name="POT6" library="pot-alps" package="ALPS_POT_VERTICAL" value="10k"/>
<element name="LDR2" library="adafruit" package="0204V" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="pinhead" package="1X04" value="">
<attribute name="VALUE"/>
</element>
<element name="R8" library="adafruit" package="0204V" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="adafruit" package="0204V" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="adafruit" package="0204V" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="T2" library="MusicThingModular" package="TO92-ECB" value="bc547">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="adafruit" package="LED5MM" value="">
<attribute name="VALUE"/>
</element>
<element name="E$1" library="special-drill" package="DRILL_0.1875" value=""/>
<element name="E$2" library="special-drill" package="DRILL_0.1875" value=""/>
<element name="E$3" library="special-drill" package="DRILL_0.1875" value=""/>
<element name="E$4" library="special-drill" package="DRILL_0.1875" value=""/>
<element name="JIN1" library="pj302m" package="PJ302M" value="PJ302M">
<attribute name="NAME"/>
</element>
<element name="D2" library="diode" package="DO41-10" value="1N4004">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JVCC1" library="adafruit" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RED" library="pinhead" package="2X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="GREEN" library="pinhead" package="2X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BLUE" library="pinhead" package="2X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C19" library="adafruit" package="C050-025X075" value="104">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JIN2" library="pj302m" package="PJ302M" value="PJ302M">
<attribute name="NAME"/>
</element>
<element name="JIN3" library="pj302m" package="PJ302M" value="PJ302M">
<attribute name="NAME"/>
</element>
<element name="O13" library="adafruit" package="1X12-CB" value="">
<attribute name="VALUE"/>
</element>
<element name="O45" library="adafruit" package="1X12-CB" value="">
<attribute name="VALUE"/>
</element>
<element name="JP1" library="adafruit" package="1X09-BIG" value="">
<attribute name="VALUE"/>
</element>
<element name="CN1" library="adafruit" package="DCJACK_2MM_PTH" value=""/>
</elements>
<signals>
<signal name="+5V">
<contactref element="IC1" pad="14"/>
<contactref element="+5V" pad="1"/>
<contactref element="LED1" pad="A"/>
<contactref element="LED2" pad="A"/>
<contactref element="C19" pad="2"/>
</signal>
<signal name="N$101">
<contactref element="C3" pad="2"/>
<contactref element="C20" pad="2"/>
<contactref element="IC1" pad="2"/>
<contactref element="JP13" pad="4"/>
<contactref element="LDR1" pad="2"/>
</signal>
<signal name="N$16">
<contactref element="C20" pad="1"/>
<contactref element="U$7" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="C3" pad="1"/>
<contactref element="U$7" pad="3"/>
</signal>
<signal name="OUT1">
<contactref element="U$7" pad="2"/>
<contactref element="O13" pad="1"/>
<contactref element="O13" pad="2"/>
<contactref element="O13" pad="3"/>
<contactref element="O13" pad="4"/>
</signal>
<signal name="N$102">
<contactref element="C14" pad="2"/>
<contactref element="C15" pad="2"/>
<contactref element="IC1" pad="4"/>
<contactref element="POT2" pad="P$2"/>
</signal>
<signal name="N$24">
<contactref element="C15" pad="1"/>
<contactref element="U$8" pad="1"/>
</signal>
<signal name="N$26">
<contactref element="C14" pad="1"/>
<contactref element="U$8" pad="3"/>
</signal>
<signal name="OUT2">
<contactref element="U$8" pad="2"/>
<contactref element="O13" pad="5"/>
<contactref element="O13" pad="6"/>
<contactref element="O13" pad="7"/>
<contactref element="O13" pad="8"/>
</signal>
<signal name="N$103">
<contactref element="C16" pad="2"/>
<contactref element="C17" pad="2"/>
<contactref element="IC1" pad="6"/>
<contactref element="POT3" pad="P$2"/>
</signal>
<signal name="N$28">
<contactref element="C17" pad="1"/>
<contactref element="U$9" pad="1"/>
</signal>
<signal name="N$29">
<contactref element="C16" pad="1"/>
<contactref element="U$9" pad="3"/>
</signal>
<signal name="OUT3">
<contactref element="U$9" pad="2"/>
<contactref element="O13" pad="9"/>
<contactref element="O13" pad="10"/>
<contactref element="O13" pad="11"/>
<contactref element="O13" pad="12"/>
</signal>
<signal name="N$104">
<contactref element="C18" pad="2"/>
<contactref element="C21" pad="2"/>
<contactref element="IC1" pad="8"/>
<contactref element="POT4" pad="P$2"/>
</signal>
<signal name="N$37">
<contactref element="C21" pad="1"/>
<contactref element="U$10" pad="1"/>
</signal>
<signal name="N$38">
<contactref element="C18" pad="1"/>
<contactref element="U$10" pad="3"/>
</signal>
<signal name="OUT4">
<contactref element="U$10" pad="2"/>
<contactref element="O45" pad="4"/>
<contactref element="O45" pad="3"/>
<contactref element="O45" pad="2"/>
<contactref element="O45" pad="1"/>
</signal>
<signal name="N$105">
<contactref element="C22" pad="2"/>
<contactref element="C23" pad="2"/>
<contactref element="IC1" pad="10"/>
<contactref element="POT5" pad="P$2"/>
</signal>
<signal name="N$40">
<contactref element="C23" pad="1"/>
<contactref element="U$11" pad="1"/>
</signal>
<signal name="N$41">
<contactref element="C22" pad="1"/>
<contactref element="U$11" pad="3"/>
</signal>
<signal name="OUT5">
<contactref element="U$11" pad="2"/>
<contactref element="O45" pad="8"/>
<contactref element="O45" pad="7"/>
<contactref element="O45" pad="6"/>
<contactref element="O45" pad="5"/>
</signal>
<signal name="N$43">
<contactref element="C25" pad="1"/>
<contactref element="U$12" pad="1"/>
</signal>
<signal name="N$44">
<contactref element="C24" pad="1"/>
<contactref element="U$12" pad="3"/>
</signal>
<signal name="OUT6">
<contactref element="U$12" pad="2"/>
<contactref element="O45" pad="12"/>
<contactref element="O45" pad="11"/>
<contactref element="O45" pad="10"/>
<contactref element="O45" pad="9"/>
</signal>
<signal name="HSYNC">
<contactref element="JHSYNC" pad="1"/>
<contactref element="JP8" pad="1"/>
<contactref element="JP3" pad="1"/>
<contactref element="JP10" pad="1"/>
<contactref element="JP9" pad="1"/>
<contactref element="JP11" pad="1"/>
<contactref element="JP12" pad="1"/>
</signal>
<signal name="VSYNC">
<contactref element="JVSYNC" pad="1"/>
<contactref element="JP8" pad="5"/>
<contactref element="JP3" pad="5"/>
<contactref element="JP9" pad="5"/>
<contactref element="JP10" pad="5"/>
<contactref element="JP11" pad="5"/>
<contactref element="JP12" pad="5"/>
</signal>
<signal name="SS1">
<contactref element="IC1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="SS2">
<contactref element="IC1" pad="3"/>
<contactref element="C4" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="SS3">
<contactref element="IC1" pad="5"/>
<contactref element="C6" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="SS4">
<contactref element="IC1" pad="9"/>
<contactref element="C8" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="SS5">
<contactref element="C10" pad="1"/>
<contactref element="C11" pad="1"/>
<contactref element="IC1" pad="11"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="SS6">
<contactref element="R8" pad="2"/>
<contactref element="C12" pad="1"/>
<contactref element="C13" pad="1"/>
<contactref element="IC1" pad="13"/>
</signal>
<signal name="N$1">
<contactref element="C1" pad="2"/>
<contactref element="U$1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="C2" pad="2"/>
<contactref element="U$1" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="C5" pad="2"/>
<contactref element="U$2" pad="3"/>
</signal>
<signal name="N$5">
<contactref element="C4" pad="2"/>
<contactref element="U$2" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="C8" pad="2"/>
<contactref element="U$4" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="C9" pad="2"/>
<contactref element="U$4" pad="3"/>
</signal>
<signal name="N$10">
<contactref element="C6" pad="2"/>
<contactref element="U$3" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="C7" pad="2"/>
<contactref element="U$3" pad="3"/>
</signal>
<signal name="N$46">
<contactref element="C10" pad="2"/>
<contactref element="U$5" pad="1"/>
</signal>
<signal name="N$48">
<contactref element="C11" pad="2"/>
<contactref element="U$5" pad="3"/>
</signal>
<signal name="N$49">
<contactref element="C13" pad="2"/>
<contactref element="U$6" pad="3"/>
</signal>
<signal name="N$50">
<contactref element="C12" pad="2"/>
<contactref element="U$6" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="LDR1" pad="1"/>
<contactref element="JP13" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="JP13" pad="3"/>
<contactref element="POT1" pad="P$2"/>
</signal>
<signal name="N$19">
<contactref element="POT1" pad="P$1"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="N$22">
<contactref element="R1" pad="2"/>
<contactref element="POT2" pad="P$1"/>
</signal>
<signal name="N$33">
<contactref element="R2" pad="2"/>
<contactref element="POT3" pad="P$1"/>
</signal>
<signal name="N$47">
<contactref element="R3" pad="2"/>
<contactref element="POT4" pad="P$1"/>
</signal>
<signal name="N$53">
<contactref element="R4" pad="2"/>
<contactref element="POT5" pad="P$1"/>
</signal>
<signal name="GND">
<contactref element="R7" pad="1"/>
<contactref element="T1" pad="E"/>
<contactref element="IC1" pad="7"/>
<contactref element="JGND" pad="1"/>
<contactref element="R10" pad="1"/>
<contactref element="T2" pad="E"/>
<contactref element="JIN1" pad="GND"/>
<contactref element="C19" pad="1"/>
<contactref element="JIN2" pad="GND"/>
<contactref element="JIN3" pad="GND"/>
<contactref element="JP12" pad="3"/>
<contactref element="JP11" pad="3"/>
<contactref element="JP10" pad="3"/>
<contactref element="JP9" pad="3"/>
<contactref element="JP8" pad="3"/>
<contactref element="JP3" pad="3"/>
<contactref element="CN1" pad="GND"/>
</signal>
<signal name="N$32">
<contactref element="R7" pad="2"/>
<contactref element="R6" pad="1"/>
<contactref element="T1" pad="B"/>
</signal>
<signal name="N$34">
<contactref element="R6" pad="2"/>
<contactref element="JP13" pad="1"/>
</signal>
<signal name="N$52">
<contactref element="LED1" pad="K"/>
<contactref element="T1" pad="C"/>
</signal>
<signal name="N$55">
<contactref element="JP2" pad="4"/>
<contactref element="LDR2" pad="2"/>
<contactref element="C24" pad="2"/>
<contactref element="C25" pad="2"/>
<contactref element="IC1" pad="12"/>
</signal>
<signal name="N$56">
<contactref element="LDR2" pad="1"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="N$57">
<contactref element="JP2" pad="3"/>
<contactref element="POT6" pad="P$2"/>
</signal>
<signal name="N$58">
<contactref element="POT6" pad="P$1"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="N$59">
<contactref element="R10" pad="2"/>
<contactref element="R9" pad="1"/>
<contactref element="T2" pad="B"/>
</signal>
<signal name="N$60">
<contactref element="R9" pad="2"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="N$61">
<contactref element="LED2" pad="K"/>
<contactref element="T2" pad="C"/>
</signal>
<signal name="VIN">
<contactref element="D2" pad="A"/>
<contactref element="CN1" pad="PWR"/>
</signal>
<signal name="N$62">
<contactref element="D2" pad="C"/>
<contactref element="JVCC1" pad="1"/>
</signal>
<signal name="ROUT">
<contactref element="RJ" pad="1"/>
<contactref element="RED" pad="1"/>
<contactref element="RED" pad="3"/>
<contactref element="RED" pad="5"/>
<contactref element="RED" pad="2"/>
<contactref element="RED" pad="4"/>
<contactref element="RED" pad="6"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="GOUT">
<contactref element="GJ" pad="1"/>
<contactref element="GREEN" pad="1"/>
<contactref element="GREEN" pad="3"/>
<contactref element="GREEN" pad="5"/>
<contactref element="GREEN" pad="6"/>
<contactref element="GREEN" pad="4"/>
<contactref element="GREEN" pad="2"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="BOUT">
<contactref element="BJ" pad="1"/>
<contactref element="BLUE" pad="1"/>
<contactref element="BLUE" pad="3"/>
<contactref element="BLUE" pad="5"/>
<contactref element="BLUE" pad="6"/>
<contactref element="BLUE" pad="4"/>
<contactref element="BLUE" pad="2"/>
<contactref element="JP1" pad="7"/>
</signal>
<signal name="N$20">
<contactref element="JP8" pad="4"/>
<contactref element="JP8" pad="2"/>
<contactref element="JP8" pad="6"/>
<contactref element="U$1" pad="2"/>
</signal>
<signal name="N$23">
<contactref element="JP9" pad="4"/>
<contactref element="JP9" pad="2"/>
<contactref element="JP9" pad="6"/>
<contactref element="U$3" pad="2"/>
</signal>
<signal name="N$31">
<contactref element="JP10" pad="4"/>
<contactref element="JP10" pad="2"/>
<contactref element="JP10" pad="6"/>
<contactref element="U$4" pad="2"/>
</signal>
<signal name="N$35">
<contactref element="JP11" pad="4"/>
<contactref element="JP11" pad="2"/>
<contactref element="JP11" pad="6"/>
<contactref element="U$5" pad="2"/>
</signal>
<signal name="N$36">
<contactref element="JP12" pad="6"/>
<contactref element="JP12" pad="4"/>
<contactref element="U$6" pad="2"/>
<contactref element="JP12" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="JP1" pad="2"/>
<contactref element="JIN1" pad="TIP"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="N$12">
<contactref element="JP1" pad="6"/>
<contactref element="JP1" pad="5"/>
<contactref element="JIN2" pad="TIP"/>
</signal>
<signal name="N$13">
<contactref element="JP1" pad="8"/>
<contactref element="JP1" pad="9"/>
<contactref element="JIN3" pad="TIP"/>
</signal>
<signal name="N$14">
<contactref element="JP3" pad="4"/>
<contactref element="JP3" pad="2"/>
<contactref element="JP3" pad="6"/>
<contactref element="U$2" pad="2"/>
</signal>
<signal name="GNDBREAK">
<contactref element="CN1" pad="GNDBREAK"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
