{"text_format":"1","workbook":"xlsx","n_sheets":11,"sheets":["Cadet I-Sync Generator.csv","Cadet II-RGB Encoder.csv","Cadet III-Video Input.csv","Cadet IV-Dual Ramp Generators.c","Cadet V-Scaler.csv","Cadet VI-Fader.csv","Cadet VII-Processor.csv","Cadet VIII-Hard Key Generator.c","Cadet IX-VCO.csv","Sheet12","Cadet 21 BOM"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":9,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1904"}

{"sheet":"Cadet I-Sync Generator.csv","index":0,"n_rows":35,"n_cols":12,"rows_kept":35,"cut":false,"hidden":false,"merged":[]}
["Line Item","Quantity","Reference Designators","Manufacturer","Manufacturer P/N","Vendor","Vendor P/N","Description","Value","Package","Part Type","Assembly Location"]
[1,1,"-","LZX Industries","LZX-C1-PCB","LZX Industries","LZX-C1-PCB","LZX Industries Cadet I Sync Generator PCB","-","-","Fabricated","-"]
[2,1,"-","LZX Industries","LZX-C1-FPN","LZX Industries","LZX-C1-FPN","LZX Industries Cadet I Sync Generator Frontpanel","-","-","Fabricated","-"]
[3,1,"C1","Vishay / Sprague","1C10Z5U334M050B ","Mouser","75-1C10Z5U334M050B ","Multilayer Ceramic Capacitors MLCC - Leaded 0.33uF 50volts Z5U 20% 2.5mm L/S","330 n","-","Through Hole","PCB Top"]
[4,13,"C3, C4, C5, C7, C8, C9, C10, C11, C13, C14, C15, C16, C22","Vishay / Sprague","1C10Z5U104M050B","Mouser","75-1C10Z5U104M050B","Multilayer Ceramic Capacitors MLCC - Leaded 0.1uF 50volts Z5U 20% 2.5mm L/S","0.1 u","-","Through Hole","PCB Top"]
[5,2,"C2, C6","Panasonic","ECE-A1VKS100","Mouser","667-ECE-A1VKS100","Aluminum Electrolytic Capacitors - Leaded 10UF 35V KS RADIAL","10 u","-","Through Hole","PCB Top"]
[6,2,"C17, C19","Vishay / BC Components","K102K15X7RH53L2","Mouser","594-K102K15X7RH53L2","Multilayer Ceramic Capacitors MLCC - Leaded 1000pF 100volts 10% X7R 2.5mm LS","1000 p","-","Through Hole","PCB Top"]
[7,1,"C18","Xicon","21RD747-RC","Mouser","21RD747-RC","Multilayer Ceramic Capacitors MLCC - Leaded 47pF 50volts C0G 5% 2.5mm L/S","47 p","-","Through Hole","PCB Top"]
[8,2,"D1, D2","Fairchild Semiconductor","1N4001","Mouser","512-1N4001","Rectifiers Vr/50V Io/1A T/R","-","-","Through Hole","PCB Top"]
[9,2,"FB1, FB2","Fair-Rite",2743001111,"Mouser","623-2743001111","EMI Filter Beads, Chips & Arrays 43 BEAD ON LEAD Z=68 OHM @ 100MHz","-","-","Through Hole","PCB Top"]
[10,6,"R2, R5, R16, R17, R20, R23","KOA Speer","MF1/4DCT52R4990F","Mouser","660-MF1/4DCT52R4990F","Metal Film Resistors - Through Hole 1/4W 499 ohm 1% 500 OHM 1%","499R","-","Through Hole","PCB Top"]
[11,1,"R10","KOA Speer","MF1/4DCT52R4992F","Mouser","660-MF1/4DCT52R4992F","Metal Film Resistors - Through Hole 1/4W 49.9K ohm 1% 500 OHM 1%","49.9K","-","Through Hole","PCB Top"]
[12,3,"R1, R3, R15","KOA Speer","MF1/4DCT52R3921F","Mouser","660-MF1/4DCT52R3921F","Metal Film Resistors - Through Hole 1/4W 3.92K ohm 1% 4.99K OHM 1%","3.92K","-","Through Hole","PCB Top"]
[13,1,"R9","KOA Speer","MF1/4DCT52R6803F","Mouser","660-MF1/4DCT52R6803F","Metal Film Resistors - Through Hole 680Kohms 1% 100PPM","680K","-","Through Hole","PCB Top"]
[14,8,"R4, R6, R11, R12, R14, R18, R26, R28","KOA Speer","MF1/4DCT52R1001F","Mouser","660-MF1/4DCT52R1001F","Metal Film Resistors - Through Hole 1Kohms 1% 100PPM","1K","-","Through Hole","PCB Top"]
[15,2,"R8, R19","KOA Speer","MF1/4DCT52R75R0F","Mouser","660-MF1/4DCT52R75R0F","Metal Film Resistors – Through Hole 1/4W 75 ohm 1% ","75R","-","Through Hole","PCB Top"]
[16,4,"R7, R21, R22, R24","KOA Speer","MF1/4DCT52R1002F","Mouser","660-MF1/4DCT52R1002F","Metal Film Resistors - Through Hole 10Kohms 1% 100PPM","10K","-","Through Hole","PCB Top"]
[17,1,"R13","TE Connectivity / Holsworthy","1623934-1","Mouser","279-1623934-1","Metal Film Resistors - Through Hole 0Ohm 1/4W LINK","0R","-","Through Hole","PCB Top"]
[18,2,"U1, U2","Texas Instruments","LM6172IN/NOPB","Mouser","926-LM6172IN/NOPB","Operational Amplifiers - Op Amps Dual High Speed,Low Pwr Amp","-","DIP8","Through Hole","PCB Top"]
[19,1,"U3","STMicroelectronics","L7805CV","Mouser","511-L7805CV","Linear Voltage Regulators 5.0V 1.0A Positive ","-","TO220","Through Hole","PCB Top"]
[20,1,"U5","Atmel","ATMEGA88A-PU","Mouser","556-ATMEGA88A-PU","8-bit Microcontrollers - MCU AVR 8KB FLSH 512B EE 1KB SRAM-20MHz","-","DIP28","Through Hole","PCB Top"]
[21,1,"U6","Texas Instruments","LM1881N/NOPB","Mouser","926-LM1881N/NOPB","Video ICs Video Sync Separator","-","DIP8","Through Hole","PCB Top"]
[22,1,"U7","Texas Instruments","SN74HC14N","Mouser","595-SN74HC14N","Inverters Hex Schmitt-Trigger ","-","DIP14","Through Hole","PCB Top"]
[23,1,"U8","Texas Instruments","CD74HC4538E","Mouser","595-CD74HC4538E","Monostable Multivibrator Dual Retrig Mono ","-","DIP16","Through Hole","PCB Top"]
[24,1,"U9","Texas Instruments","CD74HC4046AE","Mouser","595-CD74HC4046AE","Phase Locked Loops - PLL PLL w/ VCO","-","DIP16","Through Hole","PCB Top"]
[25,1,"X1","Citizen Finedevice Co Ltd","CSX750VCB13.500M-UT","DigiKey","300-8162-1-ND","OSC VCXO 13.5MHZ CMOS SMD","-","-","SMT","PCB Top"]
[26,3,"J2, J4, J6","Wenzhou QingPu","PJ302M","Thonk","MECH_JK_PJ302M","Right angled 3.5mm Jack Sockets w/Knurled Nuts, No Washers","-","-","Through Hole","PCB Top / Frontpanel"]
[27,1,"J9","-","-","Futurlec","IDCMH16 ","16 Pin Shrouded Male Headers IDC","-","-","Through Hole","PCB Top"]
[28,1,"J1","-","-","Futurlec","IDCMH14","14 Pin Shrouded Male Headers IDC","-","-","Through Hole","PCB Top"]
[29,1,"J10","-","-","Futurlec","HEADD6","6 Pin .100\" St. Male Double Headers","-","-","Through Hole","PCB Top"]
[30,2,"J3, J5","CUI","RCJ-044","Mouser","490-RCJ-044 ","RCA Phono Connectors, Right Angle, Yellow","-","-","Through Hole","PCB Top"]
[31,1,"S1","Mountain Switch","10TF230","Mouser","10TF230","Toggle Switches SPDT ON-ON RT ANGLE ","-","-","Through Hole","PCB Top / Frontpanel"]
[32,1,"M1","Keystone",621,"Mouser","534-621","Mounting Hardware THRD BRKT STL Z PL","-","-","Mechanical","PCB Top / Frontpanel"]
[33,1,"-","-","-","Erthenvar","Ribbon Cable - 16 to 16 ","16 Pin IDC EuroRack Power Cable","-","-","Accessories","-"]
[34,2,"-","-","-","McMaster-Carr","90272A106","Zinc-Plated Steel Pan Head Phillips Machine Screw, 4-40 Thread, 1/4\" Length","-","-","Mechanical","PCB Bottom / Frontpanel / M1"]

{"sheet":"Cadet II-RGB Encoder.csv","index":1,"n_rows":40,"n_cols":12,"rows_kept":40,"cut":false,"hidden":false,"merged":[]}
["Line Item","Quantity","Reference Designators","Manufacturer","Manufacturer P/N","Vendor","Vendor P/N","Description","Value","Package","Part Type","Assembly Location"]
[1,1,"-","LZX Industries","LZX-C2-PCB","LZX Industries","LZX-C2-PCB","LZX Industries Cadet II RGB Encoder PCB","-","-","Fabricated","-"]
[2,1,"-","LZX Industries","LZX-C2-FPN","LZX Industries","LZX-C2-FPN","LZX Industries Cadet II RGB Encoder Frontpanel","-","-","Fabricated","-"]
[3,1,"C1","Vishay / Sprague","1C10Z5U334M050B ","Mouser","75-1C10Z5U334M050B ","Multilayer Ceramic Capacitors MLCC - Leaded 0.33uF 50volts Z5U 20% 2.5mm L/S","330 n","-","Through Hole","PCB Top"]
[4,17,"C3, C4, C5, C7, C8, C10, C12, C13, C14, C15, C16, C22, C23, C24, C25, C26, C27","Vishay / Sprague","1C10Z5U104M050B","Mouser","75-1C10Z5U104M050B","Multilayer Ceramic Capacitors MLCC - Leaded 0.1uF 50volts Z5U 20% 2.5mm L/S","0.1 u","-","Through Hole","PCB Top"]
[5,2,"C2, C6","Panasonic","ECE-A1VKS100","Mouser","667-ECE-A1VKS100","Aluminum Electrolytic Capacitors - Leaded 10UF 35V KS RADIAL","10 u","-","Through Hole","PCB Top"]
[6,2,"C9, C11","TDK","FG18X7R1E105KRT06","Mouser","810-FG18X7R1E105KRT6","Multilayer Ceramic Capacitors MLCC - Leaded 1uF 25volts X7R +/-10% LS=2.5mm","1 u","-","Through Hole","PCB Top"]
[7,1,"C17","DNP","DNP","DNP","DNP","DNP","22:00:00","-","Through Hole","PCB Top"]
[8,2,"C18, C19","Panasonic","ECA-0JM221","Mouser","667-ECA-0JM221","Aluminum Electrolytic Capacitors - Leaded 220UF 6.3V ALUM LYTIC RADIAL","220 u","-","Through Hole","PCB Top"]
[9,2,"C20, C21","AVX","TAP106K025SCS","Mouser","581-TAP106K025SCS","Tantalum Capacitors - Solid Leaded 25volts 10uF 10%","10 u","-","Through Hole","PCB Top"]
[10,1,"C28","DNP","DNP","DNP","DNP","DNP","2.2 p – 22 p","-","Through Hole","PCB Top"]
[11,2,"D1, D2","Fairchild Semiconductor","1N4001","Mouser","512-1N4001","Rectifiers Vr/50V Io/1A T/R","-","-","Through Hole","PCB Top"]
[12,2,"D3, D4","Fairchild Semiconductor","1N4148","Mouser","512-1N4148","Diodes - General Purpose, Power, Switching 100V Io/200mA BULK","-","DO35","Through Hole","PCB Top"]
[13,12,"D5, D6, D7, D8, D9, D10, D11, D12, D13, D14, D15, D16","STMicroelectronics","1N5711","Mouser","511-1N5711","Schottky Diodes & Rectifiers 15mA 70 Volt","-","DO35","Through Hole","PCB Top"]
[14,2,"FB1, FB2","Fair-Rite",2743001111,"Mouser","623-2743001111","EMI Filter Beads, Chips & Arrays 43 BEAD ON LEAD Z=68 OHM @ 100MHz","-","-","Through Hole","PCB Top"]
[15,3,"R1, R2, R6","KOA Speer","MF1/4DCT52R4990F","Mouser","660-MF1/4DCT52R4990F","Metal Film Resistors - Through Hole 1/4W 499 ohm 1% 500 OHM 1%","499R","-","Through Hole","PCB Top"]
[16,1,"R38","KOA Speer","MF1/4DCT52R4991F","Mouser","660-MF1/4DCT52R4991F","Metal Film Resistors - Through Hole 1/4W 4.99K ohm 1% 500 OHM 1%","4.99K","-","Through Hole","PCB Top"]
[17,3,"R13, R23, R32","KOA Speer","MF1/4DCT52R1401F","Mouser","660-MF1/4DCT52R1401F","Metal Film Resistors - Through Hole 1/4W 1.4K ohm 1% ","1.4K","- ","Through Hole","PCB Top"]
[18,1,"R40","KOA Speer","MF1/4DCT52R3481F","Mouser","660-MF1/4DCT52R3481F","Metal Film Resistors - Through Hole 1/4W 3.48K ohm 1% ","3.48K","-","Through Hole","PCB Top"]
[19,3,"R3, R4, R14","KOA Speer","MF1/4DCT52R1003F","Mouser","660-MF1/4DCT52R1003F","Metal Film Resistors - Through Hole 100Kohms 1% 100PPM","100K","-","Through Hole","PCB Top"]
[20,25,"R5, R10, R11, R12, R15, R16, R17, R18, R20, R21, R22, R24, R25, R26, R27, R28, R29, R30, R31, R33, R34, R35, R36, R37, R41","KOA Speer","MF1/4DCT52R1001F","Mouser","660-MF1/4DCT52R1001F","Metal Film Resistors - Through Hole 1Kohms 1% 100PPM","1K","-","Through Hole","PCB Top"]
[21,2,"R7, R19","KOA Speer","MF1/4DCT52R75R0F","Mouser","660-MF1/4DCT52R75R0F","Metal Film Resistors – Through Hole 1/4W 75 ohm 1% ","75R","-","Through Hole","PCB Top"]
[22,2,"R8, R9","KOA Speer","MF1/4DCT52R1002F","Mouser","660-MF1/4DCT52R1002F","Metal Film Resistors - Through Hole 10Kohms 1% 100PPM","10K","-","Through Hole","PCB Top"]
[23,5,"U1, U2, U6, U8, U9","Texas Instruments","LM6172IN/NOPB","Mouser","926-LM6172IN/NOPB","Operational Amplifiers - Op Amps Dual High Speed,Low Pwr Amp","-","DIP8","Through Hole","PCB Top"]
[24,1,"U3","STMicroelectronics","L7805CV","Mouser","511-L7805CV","Linear Voltage Regulators 5.0V 1.0A Positive ","-","TO220","Through Hole","PCB Top"]
[25,1,"U7","Texas Instruments","SN74HC14N","Mouser","595-SN74HC14N","Inverters Hex Schmitt-Trigger ","-","DIP14","Through Hole","PCB Top"]
[26,1,"U4","Analog Devices","AD724JRZ","Mouser","584-AD724JRZ","Video ICs RGB-NTSC/PAL ENCODER","-","SOIC16","SMT","PCB Top"]
[27,1,"U5","Texas Instruments","CD4053BE","Mouser","595-CD4053BE","Multiplexer Switch ICs Triple 2-Ch Analog","-","DIP16","Through Hole","PCB Top"]
[28,1,"U11","Texas Instruments","TL431BQLPR","Mouser","595-TL431BQLPR","Voltage References Adjustable Precision Shunt Regulator","-","TO-92-3","Through Hole","PCB Top"]
[29,1,"Y1","ABRACON","ABL-3.579545MHZ-B2","Mouser","815-ABL-3.579545B2","Crystals +/-20ppm 3.579545MHZ FUNDAMENTAL","-","HC49","Through Hole","PCB Top"]
[30,1,"Y2","ECS","ECS-44-20-4X","Mouser","520-HCU443-20X","Crystals 4.433618MHz 20pF","-","HC49","Through Hole","PCB Top"]
[31,3,"J2, J4, J6","Wenzhou QingPu","PJ302M","Thonk","MECH_JK_PJ302M","Right angled 3.5mm Jack Sockets w/Knurled Nuts, No Washers","-","-","Through Hole","PCB Top / Frontpanel"]
[32,1,"J9","-","-","Futurlec","IDCMH16 ","16 Pin Shrouded Male Headers IDC","-","-","Through Hole","PCB Top"]
[33,1,"J1","-","-","Futurlec","IDCMH14","14 Pin Shrouded Male Headers IDC","-","-","Through Hole","PCB Top"]
[34,2,"J3, J5","CUI","RCJ-044","Mouser","490-RCJ-044 ","RCA Phono Connectors, Right Angle, Yellow","-","-","Through Hole","PCB Top"]
[35,1,"S1","Mountain Switch","10TF230","Mouser","10TF230","Toggle Switches SPDT ON-ON RT ANGLE ","-","-","Through Hole","PCB Top / Frontpanel"]
[36,1,"M1","Keystone",621,"Mouser","534-621","Mounting Hardware THRD BRKT STL Z PL","-","-","Mechanical","PCB Top / Frontpanel"]
[37,1,"-","-","-","Erthenvar","Ribbon Cable - 16 to 16 ","16 Pin IDC EuroRack Power Cable","-","-","Accessories","-"]
[38,1,"-","-","-","McMaster-Carr","90272A106","Zinc-Plated Steel Pan Head Phillips Machine Screw, 4-40 Thread, 1/4\" Length","-","-","Mechanical","PCB Bottom / Frontpanel / M1"]
[39,1,"J7","DNP","DNP","DNP","DNP","DNP","- ","-","-","-"]

{"sheet":"Cadet III-Video Input.csv","index":2,"n_rows":36,"n_cols":14,"rows_kept":36,"cut":false,"hidden":false,"merged":[]}
["Line Item","Quantity","Reference Designators","Manufacturer","Manufacturer P/N","Vendor","Vendor P/N","Description","Value","Package","Part Type","Assembly Location","Cost Each","Cost Ext"]
[1,1,"-","LZX Industries","LZX-C3-PCB","LZX Industries","LZX-C3-PCB","LZX Industries Cadet III Video Input PCB","-","-","Fabricated","-",11.53,11.53]
[2,1,"-","LZX Industries","LZX-C3-FPN","LZX Industries","LZX-C3-FPN","LZX Industries Cadet III Video Input Frontpanel","-","-","Fabricated","-",3.86,3.86]
[3,1,"C1","Vishay / Sprague","1C10Z5U334M050B ","Mouser","75-1C10Z5U334M050B ","Multilayer Ceramic Capacitors MLCC - Leaded 0.33uF 50volts Z5U 20% 2.5mm L/S","330 n","-","Through Hole","PCB Top",0.26,0.26]
[4,2,"C2, C6","Panasonic","ECE-A1VKS100","Mouser","667-ECE-A1VKS100","Aluminum Electrolytic Capacitors - Leaded 10UF 35V KS RADIAL","10 u","-","Through Hole","PCB Top",0.1,0.2]
[5,14,"C3, C4, C5, C7, C8, C9, C10, C11, C12, C13, C14, C16, C20, C22","Vishay / Sprague","1C10Z5U104M050B","Mouser","75-1C10Z5U104M050B","Multilayer Ceramic Capacitors MLCC - Leaded 0.1uF 50volts Z5U 20% 2.5mm L/S","0.1 u","-","Through Hole","PCB Top",0.24,3.36]
[6,2,"D1, D2","Fairchild Semiconductor","1N4001","Mouser","512-1N4001","Rectifiers Vr/50V Io/1A T/R","-","-","Through Hole","PCB Top",0.16,0.32]
[7,2,"D5, D6","STMicroelectronics","1N5711","Mouser","511-1N5711","Schottky Diodes & Rectifiers 15mA 70 Volt","-","DO35","Through Hole","PCB Top",0.43,0.86]
[8,2,"FB1, FB2","Fair-Rite",2743001111,"Mouser","623-2743001111","EMI Filter Beads, Chips & Arrays 43 BEAD ON LEAD Z=68 OHM @ 100MHz","-","-","Through Hole","PCB Top",0.13,0.26]
[9,1,"J2","Wenzhou QingPu","PJ302M","Thonk","MECH_JK_PJ302M","Right angled 3.5mm Jack Sockets w/Knurled Nuts, No Washers","-","-","Through Hole","PCB Top / Frontpanel",0.59,0.59]
[10,2,"J3, J4","CUI","RCJ-044","Mouser","490-RCJ-044 ","RCA Phono Connectors, Right Angle, Yellow","-","-","Through Hole","PCB Top",1.77,3.54]
[11,1,"J9","-","-","Futurlec","IDCMH16 ","16 Pin Shrouded Male Headers IDC","-","-","Through Hole","PCB Top",0.25,0.25]
[12,1,"M1","Keystone",621,"Mouser","534-621","Mounting Hardware THRD BRKT STL Z PL","-","-","Mechanical","PCB Top / Frontpanel",0.31,0.31]
[13,1,"Q1","Fairchild Semiconductor","2N3904BU","Mouser","512-2N3904BU ","Bipolar Transistors - BJT NPN Transistor General Purpose ","-","TO-92-3","Through Hole","PCB Top",0.17,0.17]
[14,2,"R1, R3","KOA Speer","MF1/4DCT52R1003F","Mouser","660-MF1/4DCT52R1003F","Metal Film Resistors - Through Hole 100Kohms 1% 100PPM","100K","-","Through Hole","PCB Top",0.12,0.24]
[15,4,"R2, R13, R15, R24","KOA Speer","MF1/4DCT52R1002F","Mouser","660-MF1/4DCT52R1002F","Metal Film Resistors - Through Hole 10Kohms 1% 100PPM","10K","-","Through Hole","PCB Top",0.12,0.48]
[16,8,"R4, R5, R7, R10, R17, R18, R20, R21","KOA Speer","MF1/4DCT52R1001F","Mouser","660-MF1/4DCT52R1001F","Metal Film Resistors - Through Hole 1Kohms 1% 100PPM","1K","-","Through Hole","PCB Top",0.12,0.96]
[17,1,"R6","KOA Speer","MF1/4DCT52R1401F","Mouser","660-MF1/4DCT52R1401F","Metal Film Resistors - Through Hole 1.4Kohms 1% 100PPM","1.4K","-","Through Hole","PCB Top",0.12,0.12]
[18,2,"R8, R19","KOA Speer","MF1/4DCT52R75R0F","Mouser","660-MF1/4DCT52R75R0F","Metal Film Resistors – Through Hole 1/4W 75 ohm 1% ","75R","-","Through Hole","PCB Top",0.12,0.24]
[19,1,"R9","KOA Speer","MF1/4DCT52R6803F","Mouser","660-MF1/4DCT52R6803F","Metal Film Resistors - Through Hole 680Kohms 1% 100PPM","680K","-","Through Hole","PCB Top",0.12,0.12]
[20,1,"R11","KOA Speer","MF1/4DCT52R2491F","Mouser","660-MF1/4DCT52R2491F","Metal Film Resistors - Through Hole 2.49Kohms 1% 100PPM","2.49K","-","Through Hole","PCB Top",0.12,0.12]
[21,2,"R12, R14","-","-","Thonk","Mech_Pot_Alpha","Right Angle B10K Alpha 9mm Potentiometer","B10K","-","Through Hole","PCB Top / Frontpanel",1.95,3.9]
[22,1,"R16","KOA Speer","MF1/4DCT52R4990F","Mouser","660-MF1/4DCT52R4990F","Metal Film Resistors - Through Hole 1/4W 499 ohm 1% ","499R","-","Through Hole","PCB Top",0.12,0.12]
[23,1,"R22","KOA Speer","MF1/4DCT52R4991F","Mouser","660-MF1/4DCT52R4991F","Metal Film Resistors - Through Hole 1/4W 4.99K ohm 1% ","4.99K","-","Through Hole","PCB Top",0.12,0.12]
[24,1,"R23","KOA Speer","MF1/4DCT52R1502F","Mouser","660-MF1/4DCT52R1502F","Metal Film Resistors - Through Hole 15Kohms 1% 100PPM","15K","-","Through Hole","PCB Top",0.12,0.12]
[25,1,"U3","STMicroelectronics","L7805CV","Mouser","511-L7805CV","Linear Voltage Regulators 5.0V 1.0A Positive ","-","TO220","Through Hole","PCB Top",0.43,0.43]
[26,1,"U4","Texas Instruments","CD4053BE","Mouser","595-CD4053BE","Multiplexer Switch ICs Triple 2-Ch Analog","-","DIP16","Through Hole","PCB Top",0.51,0.51]
[27,2,"U5, U8","Texas Instruments","LM6172IN/NOPB","Mouser","926-LM6172IN/NOPB","Operational Amplifiers - Op Amps Dual High Speed,Low Pwr Amp","-","DIP8","Through Hole","PCB Top",3.86,7.72]
[28,1,"U6","Texas Instruments","LM1881N/NOPB","Mouser","926-LM1881N/NOPB","Video ICs Video Sync Separator","-","DIP8","Through Hole","PCB Top",2.93,2.93]
[29,1,"U9","Texas Instruments","TL431BQLPR","Mouser","595-TL431BQLPR","Voltage References Adjustable Precision Shunt Regulator","-","TO-92-3","Through Hole","PCB Top",0.65,0.65]
[30,1,"U10","Texas Instruments","TL072IP","Mouser","595-TL072IP","Operational Amplifiers - Op Amps Dual JFET In Low N","-","DIP8","Through Hole","PCB Top",0.65,0.65]
[31,1,"-","-","-","Erthenvar","Ribbon Cable - 16 to 16 ","16 Pin IDC EuroRack Power Cable","-","-","Accessories","-",1.75,1.75]
[32,2,"-","-","-","McMaster-Carr","90272A106","Zinc-Plated Steel Pan Head Phillips Machine Screw, 4-40 Thread, 1/4\" Length","-","-","Mechanical","PCB Bottom / Frontpanel / M1",0.02,0.04]
[33,2,"-","-","-","Thonk","Davies_1900h","Davies 1900H Clone Red (6.35mm Round Shaft)","-","-","Control Knobs","R12, R14 shafts",0.9,1.8]
[34,1,"-","-","-","Thonk","Knurled Nuts","Knurled Nuts for PJ302M Jacks","-","-","Mechanical","Frontpanel",0.05,0.05]
["Totals",68,null,null,null,null,null,null,null,null,null,null,null,48.58]

{"sheet":"Cadet IV-Dual Ramp Generators.c","index":3,"n_rows":32,"n_cols":12,"rows_kept":32,"cut":false,"hidden":false,"merged":[]}
["Line Item","Quantity","Reference Designators","Manufacturer","Manufacturer P/N","Vendor","Vendor P/N","Description","Value","Package","Part Type","Assembly Location"]
[1,1,"-","LZX Industries","LZX-C4-PCB","LZX Industries","LZX-C4-PCB","LZX Industries Cadet IV Ramp Generator PCB","-","-","Fabricated","-"]
[2,1,"-","LZX Industries","LZX-C4-FPN","LZX Industries","LZX-C4-FPN","LZX Industries Cadet IV Ramp Generator Frontpanel","-","-","Fabricated","-"]
[3,1,"C1","Vishay / Sprague","1C10Z5U334M050B ","Mouser","75-1C10Z5U334M050B ","Multilayer Ceramic Capacitors MLCC - Leaded 0.33uF 50volts Z5U 20% 2.5mm L/S","330 n","-","Through Hole","PCB Top"]
[4,2,"C2, C6","Panasonic","ECE-A1VKS100","Mouser","667-ECE-A1VKS100","Aluminum Electrolytic Capacitors - Leaded 10UF 35V KS RADIAL","10 u","-","Through Hole","PCB Top"]
[5,12,"C3, C4, C7, C8, C9, C10, C12, C15, C16, C17, C22, C25","Vishay / Sprague","1C10Z5U104M050B","Mouser","75-1C10Z5U104M050B","Multilayer Ceramic Capacitors MLCC - Leaded 0.1uF 50volts Z5U 20% 2.5mm L/S","0.1 u","-","Through Hole","PCB Top"]
[6,2,"D1, D2","Fairchild Semiconductor","1N4001","Mouser","512-1N4001","Rectifiers Vr/50V Io/1A T/R","-","-","Through Hole","PCB Top"]
[7,4,"D3, D4, D5, D6","STMicroelectronics","1N5711","Mouser","511-1N5711","Schottky Diodes & Rectifiers 15mA 70 Volt","-","DO35","Through Hole","PCB Top"]
[8,2,"FB1, FB2","Fair-Rite",2743001111,"Mouser","623-2743001111","EMI Filter Beads, Chips & Arrays 43 BEAD ON LEAD Z=68 OHM @ 100MHz","-","-","Through Hole","PCB Top"]
[9,6,"J2, J3, J4, J6, J8, J10","Wenzhou QingPu","PJ302M","Thonk","MECH_JK_PJ302M","Right angled 3.5mm Jack Sockets w/Knurled Nuts, No Washers","-","-","Through Hole","PCB Top / Frontpanel"]
[10,1,"J9","-","-","Futurlec","IDCMH16 ","16 Pin Shrouded Male Headers IDC","-","-","Through Hole","PCB Top"]
[11,1,"J1","-","-","Futurlec","IDCMH14","14 Pin Shrouded Male Headers IDC","-","-","Through Hole","PCB Top"]
[12,2,"R27, R45","KOA Speer","MF1/4DCT52R1000F","Mouser","660-MF1/4DCT52R1000F","Metal Film Resistors - Through Hole 100 ohms 1% 100PPM","100R","-","Through Hole","PCB Top"]
[13,10,"R5, R6, R9, R10, R14, R16, R20, R24, R26, R43","KOA Speer","MF1/4DCT52R1001F","Mouser","660-MF1/4DCT52R1001F","Metal Film Resistors - Through Hole 1Kohms 1% 100PPM","1K","-","Through Hole","PCB Top"]
[14,2,"R30, R48","KOA Speer","MF1/4DCT52R2002F","Mouser","660-MF1/4DCT52R2002F","Metal Film Resistors - Through Hole 20Kohms 1% 100PPM","20K","-","Through Hole","PCB Top"]
[15,2,"R7, R11","KOA Speer","MF1/4DCT52R2001F","Mouser","660-MF1/4DCT52R2001F","Metal Film Resistors - Through Hole 2Kohms 1% 100PPM","2K","-","Through Hole","PCB Top"]
[16,10,"R8, R12, R13, R15, R18, R31, R32, R33, R49, R50","KOA Speer","MF1/4DCT52R4990F","Mouser","660-MF1/4DCT52R4990F","Metal Film Resistors - Through Hole 1/4W 499 ohm 1% ","499R","-","Through Hole","PCB Top"]
[17,5,"R2, R4, R25, R38, R44","KOA Speer","MF1/4DCT52R4991F","Mouser","660-MF1/4DCT52R4991F","Metal Film Resistors - Through Hole 1/4W 4.99K ohm 1% ","4.99K","-","Through Hole","PCB Top"]
[18,1,"R40","KOA Speer","MF1/4DCT52R1242F","Mouser","660-MF1/4DCT52R1242F","Metal Film Resistors - Through Hole 10Kohms 1% 100PPM","12.4K","-","Through Hole","PCB Top"]
[19,9,"R22, R23, R28, R29, R39, R41, R42, R46, R47","KOA Speer","MF1/4DCT52R1002F","Mouser","660-MF1/4DCT52R1002F","Metal Film Resistors - Through Hole 10Kohms 1% 100PPM","10K","-","Through Hole","PCB Top"]
[20,1,"U3","STMicroelectronics","L7805CV","Mouser","511-L7805CV","Linear Voltage Regulators 5.0V 1.0A Positive ","-","TO220","Through Hole","PCB Top"]
[21,2,"U2, U5","Texas Instruments","LM6172IN/NOPB","Mouser","926-LM6172IN/NOPB","Operational Amplifiers - Op Amps Dual High Speed,Low Pwr Amp","-","DIP8","Through Hole","PCB Top"]
[22,3,"U9, U10, U11","Texas Instruments","TL431BQLPR","Mouser","595-TL431BQLPR","Voltage References Adjustable Precision Shunt Regulator","-","TO-92-3","Through Hole","PCB Top"]
[23,1,"U1","Texas Instruments","TL072IP","Mouser","595-TL072IP","Operational Amplifiers - Op Amps Dual JFET In Low N","-","DIP8","Through Hole","PCB Top"]
[24,1,"-","-","-","Erthenvar","Ribbon Cable - 16 to 16 ","16 Pin IDC EuroRack Power Cable","-","-","Accessories","-"]
[25,2,"Q1, Q2","Fairchild Semiconductor","2N3906BU","Mouser","512-2N3906BU","Bipolar Transistors - BJT PNP Transistor General Purpose","-","TO-92-3","Through Hole","PCB Top"]
[26,1,"U7","Texas Instruments","SN74HC14N","Mouser","595-SN74HC14N","Inverters Hex Schmitt-Trigger ","-","DIP14","Through Hole","PCB Top"]
[27,2,"U12, U13","Texas Instruments","TL074CN","Mouser","595-TL074CN","Operational Amplifiers - Op Amps JFET Input Low Noise","-","DIP14","Through Hole","PCB Top"]
[28,2,"Q3, Q4","Fairchild Semiconductor","BS170","Mouser","512-BS170","MOSFET N-Channel MOSFET","-","TO-92-3","Through Hole","PCB Top"]
[29,2,"R1, R3","Bourns","3362P-1-103LF","Mouser","652-3362P-1-103LF","Trimmer Resistors - Through Hole 1/4\"SQ 10KOHMS 10% 0.5WATTS","10K","-","Through Hole","PCB Top"]
[30,1,"C18","TDK","FK11X5R1C156M","Mouser","810-FK11X5R1C156M","Multilayer Ceramic Capacitors MLCC - Leaded 15uF 16volts X5R +/-20%","15 u","-","Through Hole","PCB Top"]
[31,1,"C29","AVX","SR205C563KAA","Mouser","581-SR205C563KAA",null,"56 n","-","Through Hole","PCB Top"]

{"sheet":"Cadet V-Scaler.csv","index":4,"n_rows":18,"n_cols":12,"rows_kept":18,"cut":false,"hidden":false,"merged":[]}
["Line Item","Quantity","Reference Designators","Manufacturer","Manufacturer P/N","Vendor","Vendor P/N","Description","Value","Package","Part Type","Assembly Location"]
[1,1,"-","LZX Industries","LZX-C5-PCB","LZX Industries","LZX-C5-PCB","LZX Industries Cadet V Scaler PCB","-","-","Fabricated","-"]
[2,1,"-","LZX Industries","LZX-C5-FPN","LZX Industries","LZX-C5-FPN","LZX Industries Cadet V Scaler Frontpanel","-","-","Fabricated","-"]
[3,4,"C3, C4, C7, C8","Vishay / Sprague","1C10Z5U104M050B","Mouser","75-1C10Z5U104M050B","Multilayer Ceramic Capacitors MLCC - Leaded 0.1uF 50volts Z5U 20% 2.5mm L/S","0.1 u","-","Through Hole","PCB Top"]
[4,2,"C2, C6","Panasonic","ECE-A1VKS100","Mouser","667-ECE-A1VKS100","Aluminum Electrolytic Capacitors - Leaded 10UF 35V KS RADIAL","10 u","-","Through Hole","PCB Top"]
[5,2,"D1, D2","Fairchild Semiconductor","1N4001","Mouser","512-1N4001","Rectifiers Vr/50V Io/1A T/R","-","-","Through Hole","PCB Top"]
[6,2,"L1, L2","Fair-Rite",2743001111,"Mouser","623-2743001111","EMI Filter Beads, Chips & Arrays 43 BEAD ON LEAD Z=68 OHM @ 100MHz","-","-","Through Hole","PCB Top"]
[7,4,"R1, R3, R15, R17","KOA Speer","MF1/4DCT52R2002F","Mouser","660-MF1/4DCT52R2002F","Metal Film Resistors - Through Hole 1/4W 20K ohm 1% 20K OHM 1%","20K","-","Through Hole","PCB Top"]
[8,4,"R2, R5, R16, R19","KOA Speer","MF1/4DCT52R4990F","Mouser","660-MF1/4DCT52R4990F","Metal Film Resistors - Through Hole 1/4W 499 ohm 1% 500 OHM 1%","499R","-","Through Hole","PCB Top"]
[9,8,"R4, R6, R12, R14, R18, R20, R26, R28","KOA Speer","MF1/4DCT52R4991F","Mouser","660-MF1/4DCT52R4991F","Metal Film Resistors - Through Hole 1/4W 4.99K ohm 1% 4.99K OHM 1%","4.99K","-","Through Hole","PCB Top"]
[10,11,"R7, R8, R9, R10, R11, R13, R25, R27, R29, R30, R31","DNP","DNP","DNP","DNP","DO NOT PLACE","-","-","-","PCB Top"]
[11,2,"U1, U2","Texas Instruments","LM6172IN/NOPB","Mouser","926-LM6172IN/NOPB","Operational Amplifiers - Op Amps Dual High Speed,Low Pwr Amp","-","DIP8","Through Hole","PCB Top"]
[12,1,"U3","DNP","DNP","DNP","DNP","DO NOT PLACE","-","-","-","PCB Top"]
[13,1,"U4","DNP","DNP","DNP","DNP","DO NOT PLACE","-","-","-","PCB Top"]
[14,8,"J1, J2, J3, J4, J5, J6, J7, J8","-","-","Thonk","MECH_JK_PJ302M","Right angled 3.5mm Jack Sockets w/Knurled Nuts, No Washers","-","-","Through Hole","PCB Top / Frontpanel"]
[15,1,"J9","-","-","Futurlec","IDCMH16 ","16 Pin Shrouded Male Headers IDC","-","-","Through Hole","PCB Top"]
[16,1,"-","-","-","Erthenvar","Ribbon Cable - 16 to 16 ","16 Pin IDC EuroRack Power Cable","-","-","Accessories","-"]
[17,3,"C5, C9","DNP","DNP","DNP","DNP","DO NOT PLACE","0.1 u","-","Through Hole","PCB Top"]

{"sheet":"Cadet VI-Fader.csv","index":5,"n_rows":24,"n_cols":12,"rows_kept":24,"cut":false,"hidden":false,"merged":[]}
["Line Item","Quantity","Reference Designators","Manufacturer","Manufacturer P/N","Vendor","Vendor P/N","Description","Value","Package","Part Type","Assembly Location"]
[1,1,"-","LZX Industries","LZX-C6-PCB","LZX Industries","LZX-C6-PCB","LZX Industries Cadet VI Fader PCB","-","-","Fabricated","-"]
[2,1,"-","LZX Industries","LZX-C6-FPN","LZX Industries","LZX-C6-FPN","LZX Industries Cadet VI Fader Frontpanel","-","-","Fabricated","-"]
[3,6,"C3, C4, C5, C7, C8, C9","Vishay / Sprague","1C10Z5U104M050B","Mouser","75-1C10Z5U104M050B","Multilayer Ceramic Capacitors MLCC - Leaded 0.1uF 50volts Z5U 20% 2.5mm L/S","0.1 u","-","Through Hole","PCB Top"]
[4,2,"C2, C6","Panasonic","ECE-A1VKS100","Mouser","667-ECE-A1VKS100","Aluminum Electrolytic Capacitors - Leaded 10UF 35V KS RADIAL","10 u","-","Through Hole","PCB Top"]
[5,2,"D1, D2","Fairchild Semiconductor","1N4001","Mouser","512-1N4001","Rectifiers Vr/50V Io/1A T/R","-","-","Through Hole","PCB Top"]
[6,2,"L1, L2","Fair-Rite",2743001111,"Mouser","623-2743001111","EMI Filter Beads, Chips & Arrays 43 BEAD ON LEAD Z=68 OHM @ 100MHz","-","-","Through Hole","PCB Top"]
[7,4,"R1, R5, R12, R19","KOA Speer","MF1/4DCT52R4990F","Mouser","660-MF1/4DCT52R4990F","Metal Film Resistors - Through Hole 1/4W 499 ohm 1% 500 OHM 1%","499R","-","Through Hole","PCB Top"]
[8,2,"R2, R18","KOA Speer","MF1/4DCT52R4991F","Mouser","660-MF1/4DCT52R4991F","Metal Film Resistors - Through Hole 1/4W 4.99K ohm 1% 4.99K OHM 1%","4.99K","-","Through Hole","PCB Top"]
[9,3,"R3, R6, R14","KOA Speer","MF1/4DCT52R1003F2","Mouser","660-MF1/4DCT52R1003F","Metal Film Resistors - Through Hole 100Kohms 1% 100PPM","100K","-","Through Hole","PCB Top"]
[10,2,"R7","KOA Speer","MF1/4DCT52R1001F","Mouser","660-MF1/4DCT52R1001F","Metal Film Resistors - Through Hole 1Kohms 1% 100PPM","1K","-","Through Hole","PCB Top"]
[11,2,"R10","KOA Speer","MF1/4DCT52R6650F","Mouser","660-MF1/4DCT52R6650F","Metal Film Resistors – Through Hole 1/4W 665 ohm 1% ","665R","-","Through Hole","PCB Top"]
[12,5,"R8, R9, R11, R21, R22","KOA Speer","MF1/4DCT52R1002F","Mouser","660-MF1/4DCT52R1002F","Metal Film Resistors - Through Hole 10Kohms 1% 100PPM","10K","-","Through Hole","PCB Top"]
[13,2,"R16, R17","KOA Speer","MF1/4DCT52R1501F","Mouser","660-MF1/4DCT52R1501F","Metal Film Resistors - Through Hole 1/4W 1.5K ohm 1% 1.5K OHM 1%","1.5K","-","Through Hole","PCB Top"]
[14,2,"R4, R20","-","-","Thonk","Mech_Pot_Alpha","Right Angle B10K Alpha 9mm Potentiometer","B10K","-","Through Hole","PCB Top / Frontpanel"]
[15,2,"R13, R15","DNP","DNP","DNP","DNP","DO NOT PLACE","-","-","-","-"]
[16,1,"U1","Texas Instruments","TL072IP","Mouser","595-TL072IP","Operational Amplifiers - Op Amps Dual JFET In Low N","-","DIP8","Through Hole","PCB Top"]
[17,1,"U2","Linear Technology","LT1251CN#PBF","Linear Technology","LT1251CN#PBF","40MHz Video Fader and DC Gain Controlled Amplifier","-","DIP16","Through Hole","PCB Top"]
[18,1,"U3","Texas Instruments","LM6172IN/NOPB","Mouser","926-LM6172IN/NOPB","Operational Amplifiers - Op Amps Dual High Speed,Low Pwr Amp","-","DIP8","Through Hole","PCB Top"]
[19,1,"U4","Texas Instruments","TL431BQLPR","Mouser","595-TL431BQLPR","Voltage References Adjustable Precision Shunt Regulator","-","TO-92-3","Through Hole","PCB Top"]
[20,4,"J1, J2, J3, J4","-","-","Thonk","MECH_JK_PJ302M","Right angled 3.5mm Jack Sockets w/Knurled Nuts, No Washers","-","-","Through Hole","PCB Top / Frontpanel"]
[21,1,"J5","-","-","Futurlec","IDCMH16 ","16 Pin Shrouded Male Headers IDC","-","-","Through Hole","PCB Top"]
[22,1,"-","-","-","Erthenvar","Ribbon Cable - 16 to 16 ","16 Pin IDC EuroRack Power Cable","-","-","Accessories","-"]
[23,2,"-","-","-","Thonk","Davies_1900h","Davies 1900H Clone Red (6.35mm Round Shaft)","-","-","Control Knobs","R4, R20 shafts"]

{"sheet":"Cadet VII-Processor.csv","index":6,"n_rows":22,"n_cols":12,"rows_kept":22,"cut":false,"hidden":false,"merged":[]}
["Line Item","Quantity","Reference Designators","Manufacturer","Manufacturer P/N","Vendor","Vendor P/N","Description","Value","Package","Part Type","Assembly Location"]
[1,1,"-","LZX Industries","LZX-C7-PCB","LZX Industries","LZX-C7-PCB","LZX Industries Cadet VII Processor PCB","-","-","Fabricated","-"]
[2,1,"-","LZX Industries","LZX-C7-FPN","LZX Industries","LZX-C7-FPN","LZX Industries Cadet VII Processor Frontpanel","-","-","Fabricated","-"]
[3,2,"C2, C6","Panasonic","ECE-A1VKS100","Mouser","667-ECE-A1VKS100","Aluminum Electrolytic Capacitors - Leaded 10UF 35V KS RADIAL","10 u","-","Through Hole","PCB Top"]
[4,6,"C3, C4, C5, C7, C8, C9","Vishay / Sprague","1C10Z5U104M050B","Mouser","75-1C10Z5U104M050B","Multilayer Ceramic Capacitors MLCC - Leaded 0.1uF 50volts Z5U 20% 2.5mm L/S","0.1 u","-","Through Hole","PCB Top"]
[5,2,"D1, D2","Fairchild Semiconductor","1N4001","Mouser","512-1N4001","Rectifiers Vr/50V Io/1A T/R","-","-","Through Hole","PCB Top"]
[6,2,"FB1, FB2","Fair-Rite",2743001111,"Mouser","623-2743001111","EMI Filter Beads, Chips & Arrays 43 BEAD ON LEAD Z=68 OHM @ 100MHz","-","-","Through Hole","PCB Top"]
[7,3,"J1, J3, J4","Wenzhou QingPu","PJ302M","Thonk","MECH_JK_PJ302M","Right angled 3.5mm Jack Sockets w/Knurled Nuts, No Washers","-","-","Through Hole","PCB Top / Frontpanel"]
[8,1,"J5","-","-","Futurlec","IDCMH16 ","16 Pin Shrouded Male Headers IDC","-","-","Through Hole","PCB Top"]
[9,2,"R3, R14","KOA Speer","MF1/4DCT52R1003F","Mouser","660-MF1/4DCT52R1003F","Metal Film Resistors - Through Hole 100K ohms 1% 100PPM","100K","-","Through Hole","PCB Top"]
[10,9,"R2, R5, R6, R7, R10, R11, R13, R15, R16","KOA Speer","MF1/4DCT52R1001F","Mouser","660-MF1/4DCT52R1001F","Metal Film Resistors - Through Hole 1Kohms 1% 100PPM","1K","-","Through Hole","PCB Top"]
[11,1,"R22","KOA Speer","MF1/4DCT52R2002F","Mouser","660-MF1/4DCT52R2002F","Metal Film Resistors - Through Hole 20Kohms 1% 100PPM","20K","-","Through Hole","PCB Top"]
[12,3,"R1, R12, R19","KOA Speer","MF1/4DCT52R4990F","Mouser","660-MF1/4DCT52R4990F","Metal Film Resistors - Through Hole 1/4W 499 ohm 1% ","499R","-","Through Hole","PCB Top"]
[13,2,"R18, R21","KOA Speer","MF1/4DCT52R4991F","Mouser","660-MF1/4DCT52R4991F","Metal Film Resistors - Through Hole 1/4W 4.99K ohm 1% ","4.99K","-","Through Hole","PCB Top"]
[14,2,"R8, R9","KOA Speer","MF1/4DCT52R1002F","Mouser","660-MF1/4DCT52R1002F","Metal Film Resistors - Through Hole 10Kohms 1% 100PPM","10K","-","Through Hole","PCB Top"]
[15,2,"U2, U3","Texas Instruments","LM6172IN/NOPB","Mouser","926-LM6172IN/NOPB","Operational Amplifiers - Op Amps Dual High Speed,Low Pwr Amp","-","DIP8","Through Hole","PCB Top"]
[16,1,"U4","Texas Instruments","TL431BQLPR","Mouser","595-TL431BQLPR","Voltage References Adjustable Precision Shunt Regulator","-","TO-92-3","Through Hole","PCB Top"]
[17,1,null,"-","-","Erthenvar","Ribbon Cable - 16 to 16 ","16 Pin IDC EuroRack Power Cable","-","-","Accessories","-"]
[18,1,"U5","Texas Instruments","TL074CN","Mouser","595-TL074CN","Operational Amplifiers - Op Amps JFET Input Low Noise","-","DIP14","Through Hole","PCB Top"]
[19,2,"-","-","-","Thonk","Davies_1900h","Davies 1900H Clone Red (6.35mm Round Shaft)","-","-","Control Knobs","R4, R20 shafts"]
[20,2,"R4, R20","-","-","Thonk","Mech_Pot_Alpha","Right Angle B10K Alpha 9mm Potentiometer","B10K","-","Through Hole","PCB Top / Frontpanel"]
[21,1,"S1","C&K Components","7201MD9ABE","Mouser","611-7201-051","Toggle Switches ON-ON DPDT RA PC","-","-","Through Hole","PCB Top / Frontpanel"]

{"sheet":"Cadet VIII-Hard Key Generator.c","index":7,"n_rows":25,"n_cols":12,"rows_kept":25,"cut":false,"hidden":false,"merged":[]}
["Line Item","Quantity","Reference Designators","Manufacturer","Manufacturer P/N","Vendor","Vendor P/N","Description","Value","Package","Part Type","Assembly Location"]
[1,1,"-","LZX Industries","LZX-C8-PCB","LZX Industries","LZX-C8-PCB","LZX Industries Cadet VIII Hard Key Generator PCB","-","-","Fabricated","-"]
[2,1,"-","LZX Industries","LZX-C8-FPN","LZX Industries","LZX-C8-FPN","LZX Industries Cadet VIII Hard Key Generator Frontpanel","-","-","Fabricated","-"]
[3,2,"C2, C6","Panasonic","ECE-A1VKS100","Mouser","667-ECE-A1VKS100","Aluminum Electrolytic Capacitors - Leaded 10UF 35V KS RADIAL","10 u","-","Through Hole","PCB Top"]
[4,10,"C3, C4, C5, C7, C8, C9, C10, C12, C13, C22","Vishay / Sprague","1C10Z5U104M050B","Mouser","75-1C10Z5U104M050B","Multilayer Ceramic Capacitors MLCC - Leaded 0.1uF 50volts Z5U 20% 2.5mm L/S","0.1 u","-","Through Hole","PCB Top"]
[5,2,"D1, D2","Fairchild Semiconductor","1N4001","Mouser","512-1N4001","Rectifiers Vr/50V Io/1A T/R","-","-","Through Hole","PCB Top"]
[6,2,"L1, L2","Fair-Rite",2743001111,"Mouser","623-2743001111","EMI Filter Beads, Chips & Arrays 43 BEAD ON LEAD Z=68 OHM @ 100MHz","-","-","Through Hole","PCB Top"]
[7,4,"J1, J2, J3, J4","Wenzhou QingPu","PJ302M","Thonk","MECH_JK_PJ302M","Right angled 3.5mm Jack Sockets w/Knurled Nuts, No Washers","-","-","Through Hole","PCB Top / Frontpanel"]
[8,1,"J5","-","-","Futurlec","IDCMH16 ","16 Pin Shrouded Male Headers IDC","-","-","Through Hole","PCB Top"]
[9,3,"R3, R10, R14","KOA Speer","MF1/4DCT52R1003F","Mouser","660-MF1/4DCT52R1003F","Metal Film Resistors - Through Hole 100K ohms 1% 100PPM","100K","-","Through Hole","PCB Top"]
[10,5,"R5, R7, R15, R17, R24","KOA Speer","MF1/4DCT52R1001F","Mouser","660-MF1/4DCT52R1001F","Metal Film Resistors - Through Hole 1Kohms 1% 100PPM","1K","-","Through Hole","PCB Top"]
[11,4,"R1, R12, R16, R25","KOA Speer","MF1/4DCT52R4990F","Mouser","660-MF1/4DCT52R4990F","Metal Film Resistors - Through Hole 1/4W 499 ohm 1% ","499R","-","Through Hole","PCB Top"]
[12,7,"R2, R8, R9, R11, R18, R22, R26","KOA Speer","MF1/4DCT52R4991F","Mouser","660-MF1/4DCT52R4991F","Metal Film Resistors - Through Hole 1/4W 4.99K ohm 1% ","4.99K","-","Through Hole","PCB Top"]
[13,2,"R21, R27","KOA Speer","MF1/4DCT52R1002F","Mouser","660-MF1/4DCT52R1002F","Metal Film Resistors - Through Hole 10Kohms 1% 100PPM","10K","-","Through Hole","PCB Top"]
[14,2,"R6, R19","KOA Speer","MF1/4DCT52R2321F","Mouser","660-MF1/4DCT52R2321F","Metal Film Resistors - Through Hole 2.32Kohms 1% 100PPM","2.32K","-","Through Hole","PCB Top"]
[15,2,"R13, R23","KOA Speer","MF1/4DCT52R4992F","Mouser","660-MF1/4DCT52R4992F","Metal Film Resistors - Through Hole 49.9Kohms 1% 100PPM","49.9K","-","Through Hole","PCB Top"]
[16,2,"U3, U6","Texas Instruments","LM6172IN/NOPB","Mouser","926-LM6172IN/NOPB","Operational Amplifiers - Op Amps Dual High Speed,Low Pwr Amp","-","DIP8","Through Hole","PCB Top"]
[17,1,"U4","Texas Instruments","TL431BQLPR","Mouser","595-TL431BQLPR","Voltage References Adjustable Precision Shunt Regulator","-","TO-92-3","Through Hole","PCB Top"]
[18,1,"U1","Texas Instruments","TL072IP","Mouser","595-TL072IP","Operational Amplifiers - Op Amps Dual JFET In Low N","-","DIP8","Through Hole","PCB Top"]
[19,2,"R4, R20","-","-","Thonk","Mech_Pot_Alpha","Right Angle B10K Alpha 9mm Potentiometer","B10K","-","Through Hole","PCB Top / Frontpanel"]
[20,1,"C1","Vishay / Sprague","1C10Z5U334M050B ","Mouser","75-1C10Z5U334M050B ","Multilayer Ceramic Capacitors MLCC - Leaded 0.33uF 50volts Z5U 20% 2.5mm L/S","330 n","-","Through Hole","PCB Top"]
[21,1,"U5","STMicroelectronics","L7805CV","Mouser","511-L7805CV","Linear Voltage Regulators 5.0V 1.0A Positive ","-","TO220","Through Hole","PCB Top"]
[22,2,"-","-","-","Thonk","Davies_1900h","Davies 1900H Clone Red (6.35mm Round Shaft)","-","-","Control Knobs","R4, R20 shafts"]
[23,1,"U2","Texas Instruments","LM361N/NOPB","Mouser","926-LM361N/NOPB","Analog Comparators Hi Speed Diff Cmptr","-","DIP14","Through Hole","PCB Top"]
[24,1,"-","-","-","Erthenvar","Ribbon Cable - 16 to 16 ","16 Pin IDC EuroRack Power Cable","-","-","Accessories","-"]

{"sheet":"Cadet IX-VCO.csv","index":8,"n_rows":50,"n_cols":12,"rows_kept":50,"cut":false,"hidden":false,"merged":[]}
["* Q5A/Q5B, Q2A/Q2B, Q4A/Q4B must be matched transistor pairs.  We recommend sourcing these from Thonk.co.uk if you do not have the capability of matching transistors."]
["** R43 may be a 2K TempCo resistor. Not required for a video oscillator."]
["Line Item","Quantity","Reference Designators","Manufacturer","Manufacturer P/N","Vendor","Vendor P/N","Description","Value","Package","Part Type","Assembly Location"]
[1,1,"-","LZX Industries","LZX-C9-PCB","LZX Industries","LZX-C9-PCB","LZX Industries Cadet IX VCO PCB","-","-","Fabricated","-"]
[2,1,"-","LZX Industries","LZX-C9-FPN","LZX Industries","LZX-C9-FPN","LZX Industries Cadet IX VCO Frontpanel","-","-","Fabricated","-"]
[3,2,"C4, C8","Panasonic","ECE-A1VKS100","Mouser","667-ECE-A1VKS100","Aluminum Electrolytic Capacitors - Leaded 10UF 35V KS RADIAL","10 u","-","Through Hole","PCB Top"]
[4,11,"C9, C14, C15, C24, C25, C26, C27, C28, C29, C30, C54","Vishay / Sprague","1C10Z5U104M050B","Mouser","75-1C10Z5U104M050B","Multilayer Ceramic Capacitors MLCC - Leaded 0.1uF 50volts Z5U 20% 2.5mm L/S","0.1 u","-","Through Hole","PCB Top"]
[5,2,"D7, D8","Fairchild Semiconductor","1N4001","Mouser","512-1N4001","Rectifiers Vr/50V Io/1A T/R","-","-","Through Hole","PCB Top"]
[6,3,"FB3, FB4, FB5","Fair-Rite",2743001111,"Mouser","623-2743001111","EMI Filter Beads, Chips & Arrays 43 BEAD ON LEAD Z=68 OHM @ 100MHz","-","-","Through Hole","PCB Top"]
[7,2,"J1, J4","Wenzhou QingPu","PJ302M","Thonk","MECH_JK_PJ302M","Right angled 3.5mm Jack Sockets w/Knurled Nuts, No Washers","-","-","Through Hole","PCB Top / Frontpanel"]
[8,1,"J9","-","-","Futurlec","IDCMH16 ","16 Pin Shrouded Male Headers IDC","-","-","Through Hole","PCB Top"]
[9,1,"R144","KOA Speer","MF1/4DCT52R1003F","Mouser","660-MF1/4DCT52R1003F","Metal Film Resistors - Through Hole 100K ohms 1% 100PPM","100K","-","Through Hole","PCB Top"]
[10,10,"R7, R9, R23, R27, R32, R104, R111, R112, R146, R166","KOA Speer","MF1/4DCT52R1001F","Mouser","660-MF1/4DCT52R1001F","Metal Film Resistors - Through Hole 1Kohms 1% 100PPM","1K","-","Through Hole","PCB Top"]
[11,5,"R1, R10, R11, R145, R150","KOA Speer","MF1/4DCT52R4990F","Mouser","660-MF1/4DCT52R4990F","Metal Film Resistors - Through Hole 1/4W 499 ohm 1% ","499R","-","Through Hole","PCB Top"]
[12,3,"R18, R147, R148","KOA Speer","MF1/4DCT52R4991F","Mouser","660-MF1/4DCT52R4991F","Metal Film Resistors - Through Hole 1/4W 4.99K ohm 1% ","4.99K","-","Through Hole","PCB Top"]
[13,1,"R5","KOA Speer","MF1/4DCT52R1002F","Mouser","660-MF1/4DCT52R1002F","Metal Film Resistors - Through Hole 10Kohms 1% 100PPM","10K","-","Through Hole","PCB Top"]
[14,1,"R164","KOA Speer","MF1/4DCT52R2211F","Mouser","660-MF1/4DCT52R2211F","Metal Film Resistors - Through Hole 2.21Kohms 1% 100PPM","2.21K","-","Through Hole","PCB Top"]
[15,1,"R107","KOA Speer","MF1/4DCT52R4992F","Mouser","660-MF1/4DCT52R4992F","Metal Film Resistors - Through Hole 49.9Kohms 1% 100PPM","49.9K","-","Through Hole","PCB Top"]
[16,2,"U10, U20","Texas Instruments","LM6172IN/NOPB","Mouser","926-LM6172IN/NOPB","Operational Amplifiers - Op Amps Dual High Speed,Low Pwr Amp","-","DIP8","Through Hole","PCB Top"]
[17,1,"U4","Texas Instruments","TL431BQLPR","Mouser","595-TL431BQLPR","Voltage References Adjustable Precision Shunt Regulator","-","TO-92-3","Through Hole","PCB Top"]
[18,2,"U1, U9","Texas Instruments","TL072IP","Mouser","595-TL072IP","Operational Amplifiers - Op Amps Dual JFET In Low N","-","DIP8","Through Hole","PCB Top"]
[19,2,"R4, R20","-","-","Thonk","Mech_Pot_Alpha","Right Angle B10K Alpha 9mm Potentiometer","B10K","-","Through Hole","PCB Top / Frontpanel"]
[20,1,"C3","Vishay / Sprague","1C10Z5U334M050B ","Mouser","75-1C10Z5U334M050B ","Multilayer Ceramic Capacitors MLCC - Leaded 0.33uF 50volts Z5U 20% 2.5mm L/S","330 n","-","Through Hole","PCB Top"]
[21,1,"U5","STMicroelectronics","L7805CV","Mouser","511-L7805CV","Linear Voltage Regulators 5.0V 1.0A Positive ","-","TO220","Through Hole","PCB Top"]
[22,2,"-","-","-","Thonk","Davies_1900h","Davies 1900H Clone Red (6.35mm Round Shaft)","-","-","Control Knobs","R4, R20 shafts"]
[23,1,"-","-","-","Erthenvar","Ribbon Cable - 16 to 16 ","16 Pin IDC EuroRack Power Cable","-","-","Accessories","-"]
[24,2,"-","-","-","Thonk","Knurled Nuts","Knurled Nuts for PJ302M Jacks","-","-","Mechanical","Frontpanel"]
[25,1,"U12","Texas Instruments","SN74HC14N","Mouser","595-SN74HC14N","Inverters Hex Schmitt-Trigger ","-","DIP14","Through Hole","PCB Top"]
[26,1,"C23","Vishay / BC Components","K102K15X7RH53L2","Mouser","594-K102K15X7RH53L2","Multilayer Ceramic Capacitors MLCC - Leaded 1000pF 100volts 10% X7R 2.5mm LS","1000 p","-","Through Hole","PCB Top"]
[27,1,"J2","-","-","Futurlec","IDCMH14","14 Pin Shrouded Male Headers IDC","-","-","Through Hole","PCB Top"]
[28,2,"D4, D6","Fairchild Semiconductor","1N4148","Mouser","512-1N4148","Diodes - General Purpose, Power, Switching 100V Io/200mA BULK","-","DO35","Through Hole","PCB Top"]
[29,1,"S2","Mountain Switch","10TF230","Mouser","10TF230","Toggle Switches SPDT ON-ON RT ANGLE ","-","-","Through Hole","PCB Top / Frontpanel"]
[30,2,"Q5A*, Q5B*","Fairchild Semiconductor","2N3906BU","Mouser","512-2N3906BU","Bipolar Transistors - BJT PNP Transistor General Purpose","-","TO-92-3","Through Hole","PCB Top"]
[31,4,"Q2A*, Q2B*, Q4A*, Q4B*","Fairchild Semiconductor","2N3904BU","Mouser","512-2N3904BU ","Bipolar Transistors - BJT NPN Transistor General Purpose","-","TO-92-3","Through Hole","PCB Top"]
[32,1,"S1","C&K Components","7201MD9ABE","Mouser","611-7201-051","Toggle Switches ON-ON DPDT RA PC","-","-","Through Hole","PCB Top / Frontpanel"]
[33,1,"R6","Bourns","3362P-1-103LF","Mouser","652-3362P-1-103LF","Trimmer Resistors - Through Hole 1/4\"SQ 10KOHMS 10% 0.5WATTS","10K","-","Through Hole","PCB Top"]
[34,1,"R41","KOA Speer","MF1/4DCT52R1000F","Mouser","660-MF1/4DCT52R1000F","Metal Film Resistors - Through Hole 100 ohms 1% 100PPM","100R","-","Through Hole","PCB Top"]
[35,2,"R42, R113","KOA Speer","MF1/4DCT52R75R0F","Mouser","660-MF1/4DCT52R75R0F","Metal Film Resistors ï¿½ Through Hole 1/4W 75 ohm 1% ","75R","-","Through Hole","PCB Top"]
[36,1,"R43**","KOA Speer","MF1/4DCT52R2001F","Mouser","660-MF1/4DCT52R2001F","Metal Film Resistors - Through Hole 2Kohms 1% 100PPM","2K","-","Through Hole","PCB Top"]
[37,2,"R2, R30","KOA Speer","MF1/4DCT52R1652F","Mouser","660-MF1/4DCT52R1652F","Metal Film Resistors - Through Hole 16.5Kohms 1% 100PPM","16.5K","-","Through Hole","PCB Top"]
[38,3,"R3, R8, R25","KOA Speer","MF1/4DCT52R4021F","Mouser","660-MF1/4DCT52R4021F","Metal Film Resistors - Through Hole 4.02Kohms 1% 100PPM","4.02K","-","Through Hole","PCB Top"]
[39,1,"R46","KOA Speer","MF1/4DCT52R8251F","Mouser","660-MF1/4DCT52R8251F","Metal Film Resistors - Through Hole 8.25Kohms 1% 100PPM","8.25K","-","Through Hole","PCB Top"]
[40,1,"R47","KOA Speer","MF1/4DCT52R1204F","Mouser","660-MF1/4DCT52R1204F","Metal Film Resistors - Through Hole 1.2M ohms 1% 100PPM","1.2M","-","Through Hole","PCB Top"]
[41,1,"R106","KOA Speer","MF1/4DCT52R2051F","Mouser","660-MF1/4DCT52R2051F","Metal Film Resistors - Through Hole 2.05Kohms 1% 100PPM","2.05K","-","Through Hole","PCB Top"]
[42,1,"C13","Vishay / BC Components","K101J15C0GF53L2","Mouser","594-K101J15C0GF53L2","Multilayer Ceramic Capacitors MLCC - Leaded 100pF 50volts 5% .1LS C0G/NPO","100p","-","Through Hole","PCB Top"]
[43,1,"C16","Vishay / BC Components","K151J15C0GF53L2","Mouser","594-K151J15C0GF53L2","Multilayer Ceramic Capacitors MLCC - Leaded 100pF 50volts 5% .1LS C0G/NPO","150p","-","Through Hole","PCB Top"]
[44,1,"C17","TDK","FK16C0G1H473J","Mouser","810-FK16C0G1H473J","Multilayer Ceramic Capacitors MLCC - Leaded 0.047uF 50volts C0G +/-5%","47nF","-","Through Hole","PCB Top"]
[45,1,"C18","TDK","FG18C0G1H150JNT00","Mouser","810-FG18C0G1H150JNT0","Multilayer Ceramic Capacitors MLCC - Leaded 15pF 50volts C0G 5% Radial LS:2.5mm","15pF","-","Through Hole","PCB Top"]
[46,1,"C22","TDK","FG18X5R1H105KRT00","Mouser","810-FG18X5R1H105KRT0","Multilayer Ceramic Capacitors MLCC - Leaded 1uF 50volts X5R 10% Radial LS:2.5mm","1uF","-","Through Hole","PCB Top"]
[47,1,"U11","Texas Instruments","CD4066BE","Mouser","595-CD4066BE","Analog Switch ICs Quad","-","DIP-14","Through Hole","PCB Top"]

{"sheet":"Sheet12","index":9,"n_rows":75,"n_cols":10,"rows_kept":75,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[]
[]
["CADET 21 BOM"]
["Mouser #","Mfr. #","Manufacturer","Customer #","Description","RoHS","Lifecycle","Order Qty.","Price (USD)","Ext.: (USD)"]
["75-1C10Z5U334M050B","1C10Z5U334M050B","Vishay",null,"Multilayer Ceramic Capacitors MLCC - Leaded 0.33uF 50volts Z5U 20% 2.5mm L/S","RoHS Compliant By Exemption",null,12,"$0.26","$3.12"]
["75-1C10Z5U104M050B","1C10Z5U104M050B","Vishay",null,"Multilayer Ceramic Capacitors MLCC - Leaded 0.1uF 50volts Z5U 20% 2.5mm L/S","RoHS Compliant By Exemption",null,117,"$0.073","$8.54"]
["667-ECE-A1VKS100","ECE-A1VKS100","Panasonic",null,"Aluminum Electrolytic Capacitors - Leaded 10UF 35V KS RADIAL","RoHS Compliant",null,33,"$0.103","$3.40"]
["594-K102K15X7RH53L2","K102K15X7RH53L2","Vishay",null,"Multilayer Ceramic Capacitors MLCC - Leaded 1000pF 100volts 10% X7R 2.5mm LS","RoHS Compliant By Exemption",null,5,"$0.10","$0.50"]
["21RD747-RC","21RD747-RC","Xicon",null,"Multilayer Ceramic Capacitors MLCC - Leaded 47pF 50volts C0G 5% 2.5mm L/S","RoHS Compliant",null,1,"$0.10","$0.10"]
["623-2743001111","2743001111","Fair-Rite",null,"Ferrite Beads 43 BEAD ON LEAD Z=68 OHM @ 100MHz","RoHS Compliant",null,37,"$0.13","$4.81"]
["660-MF1/4DCT52R4990F","MF1/4DCT52R4990F","KOA Speer",null,"Metal Film Resistors - Through Hole 1/4W 499 ohm 1% 500 OHM 1%","RoHS Compliant",null,57,"$0.12","$6.84"]
["660-MF1/4DCT52R4992F","MF1/4DCT52R4992F","KOA Speer",null,"Metal Film Resistors - Through Hole 1/4W 49.9K ohm 1% 49.9K OHM 1%","RoHS Compliant",null,13,"$0.12","$1.56"]
["660-MF1/4DCT52R3921F","MF1/4DCT52R3921F","KOA Speer",null,"Metal Film Resistors - Through Hole 1/4W 3.92K ohm 1% 3.91K OHM 1%","RoHS Compliant",null,1,"$0.12","$0.12"]
["660-MF1/4DCT52R6803F","MF1/4DCT52R6803F","KOA Speer",null,"Metal Film Resistors - Through Hole 1/4 WATT 680K OHM 1%","RoHS Compliant",null,2,"$0.12","$0.24"]
["660-MF1/4DCT52R1001F","MF1/4DCT52R1001F","KOA Speer",null,"Metal Film Resistors - Through Hole 1Kohms 1% 100PPM","RoHS Compliant",null,104,"$0.12","$12.48"]
["660-MF1/4DCT52R75R0F","MF1/4DCT52R75R0F2","KOA Speer",null,"Metal Film Resistors - Through Hole 75ohms 1% 100PPM","RoHS Compliant",null,11,"$0.12","$1.32"]
["660-MF1/4DCT52R1002F","MF1/4DCT52R1002F","KOA Speer",null,"Metal Film Resistors - Through Hole 10Kohms 1% 100PPM","RoHS Compliant",null,28,"$0.12","$3.36"]
["279-1623934-1","1623934-1","TE Connectivity",null,"Metal Film Resistors - Through Hole 0Ohm 1/4W LINK","RoHS Compliant",null,1,"$0.10","$0.10"]
["926-LM6172IN/NOPB","LM6172IN/NOPB","Texas Instruments",null,"High Speed Operational Amplifiers Dual High Speed,Low Pwr Amp","RoHS Compliant",null,33,"$3.19","$105.27"]
["511-L7805CV","L7805CV","STMicroelectronics",null,"Linear Voltage Regulators 5.0V 1.0A Positive","RoHS Compliant",null,12,"$0.361","$4.33"]
["556-ATMEGA88A-PU","ATMEGA88A-PU","Atmel",null,"8-bit Microcontrollers - MCU AVR 8KB FLSH 512B EE 1KB SRAM-20MHz","RoHS Compliant",null,1,"$3.24","$3.24"]
["926-LM1881N/NOPB","LM1881N/NOPB","Texas Instruments",null,"Video ICs Video Sync Separator","RoHS Compliant",null,2,"$2.93","$5.86"]
["595-SN74HC14N","SN74HC14N","Texas Instruments",null,"Inverters Hex Schmitt-Trigger","RoHS Compliant",null,7,"$0.54","$3.78"]
["595-CD74HC4538E","CD74HC4538E","Texas Instruments",null,"Monostable Multivibrator Dual Retrig Mono","RoHS Compliant",null,1,"$0.73","$0.73"]
["595-CD74HC4046AE","CD74HC4046AE","Texas Instruments",null,"Phase Locked Loops - PLL PLL w/ VCO","RoHS Compliant",null,1,"$0.61","$0.61"]
["490-RCJ-044","RCJ-044","CUI Inc.",null,"RCA Phono Connectors RCA Connectors","RoHS Compliant","New At Mouser",3,"$1.77","$5.31"]
["534-621","621","Keystone Electronics",null,"Mounting Hardware THRD BRKT STL Z PL","RoHS Compliant",null,3,"$0.31","$0.93"]
["810-FG18X7R1E105KRT6","FG18X7R1E105KRT06","TDK",null,"Multilayer Ceramic Capacitors MLCC - Leaded 1uF 25volts X7R +/-10% LS=2.5mm","RoHS Compliant","New Product",1,"$0.38","$0.38"]
["667-ECA-0JM221","ECA-0JM221","Panasonic",null,"Aluminum Electrolytic Capacitors - Leaded 220UF 6.3V ALUM LYTIC RADIAL","RoHS Compliant",null,1,"$0.20","$0.20"]
["581-TAP106K025SCS","TAP106K025SCS","AVX",null,"Tantalum Capacitors - Solid Leaded 25volts 10uF 10%","RoHS Compliant",null,1,"$0.60","$0.60"]
["512-1N4148","1N4148","Fairchild Semiconductor",null,"Diodes - General Purpose, Power, Switching 100V Io/200mA BULK","RoHS Compliant",null,9,"$0.10","$0.90"]
["511-1N5711","1N5711","STMicroelectronics",null,"Schottky Diodes & Rectifiers 15mA 70 Volt","RoHS Compliant",null,3,"$0.44","$1.32"]
["660-MF1/4DCT52R4991F","MF1/4DCT52R4991F","KOA Speer",null,"Metal Film Resistors - Through Hole 1/4W 4.99K ohm 1% 4.99K OHM 1%","RoHS Compliant",null,56,"$0.12","$6.72"]
["660-MF1/4DCT52R1401F","MF1/4DCT52R1401F","KOA Speer",null,"Metal Film Resistors - Through Hole 1/4W 1.4K ohm 1%","RoHS Compliant",null,2,"$0.12","$0.24"]
["660-MF1/4DCT52R3481F","MF1/4DCT52R3481F","KOA Speer",null,"Metal Film Resistors - Through Hole 1/4W 3.48K ohm 1% 3.48K OHM 1%","RoHS Compliant",null,1,"$0.12","$0.12"]
["660-MF1/4DCT52R1003F","MF1/4DCT52R1003F2","KOA Speer",null,"Metal Film Resistors - Through Hole 100Kohms 1% 100PPM","RoHS Compliant","End of Life",30,"$0.12","$3.60"]
["584-AD724JRZ","AD724JRZ","Analog Devices Inc.",null,"Video ICs RGB-NTSC/PAL ENCODER","RoHS Compliant",null,1,"$14.61","$14.61"]
["595-CD4053BE","CD4053BE","Texas Instruments",null,"Multiplexer Switch ICs Triple 2-Ch Analog","RoHS Compliant",null,2,"$0.51","$1.02"]
["595-TL431BQLPR","TL431BQLPR","Texas Instruments",null,"Voltage References Adjustable Precision Shunt Regulator","RoHS Compliant",null,19,"$0.491","$9.33"]
["815-ABL-3.579545B2","ABL-3.579545MHZ-B2","ABRACON",null,"Crystals +/-20ppm 3.579545MHZ FUNDAMENTAL","RoHS Compliant",null,1,"$0.34","$0.34"]
["520-HCU443-20X","ECS-44-20-4X","ECS",null,"Crystals 4.433618MHz 20pF","RoHS Compliant",null,1,"$0.69","$0.69"]
["512-2N3904BU","2N3904BU","Fairchild Semiconductor",null,"Bipolar Transistors - BJT NPN Transistor General Purpose","RoHS Compliant",null,17,"$0.162","$2.75"]
["660-MF1/4DCT52R2491F","MF1/4DCT52R2491F2","KOA Speer",null,"Metal Film Resistors - Through Hole 2.49Kohms 1% 100PPM","RoHS Compliant",null,1,"$0.12","$0.12"]
["660-MF1/4DCT52R1502F","MF1/4DCT52R1502F","KOA Speer",null,"Metal Film Resistors - Through Hole 1/4W 15K ohm 1% 15K OHM 1%","RoHS Compliant",null,1,"$0.12","$0.12"]
["595-TL072IP","TL072IP","Texas Instruments",null,"Operational Amplifiers - Op Amps Dual JFET In Low N","RoHS Compliant",null,18,"$0.546","$9.83"]
["660-MF1/4DCT52R1000F","MF1/4DCT52R1000F2","KOA Speer",null,"Metal Film Resistors - Through Hole 100ohms 1% 100PPM","RoHS Compliant",null,5,"$0.12","$0.60"]
["660-MF1/4DCT52R2002F","MF1/4DCT52R2002F","KOA Speer",null,"Metal Film Resistors - Through Hole 1/4W 20K ohm 1% 20K OHM 1%","RoHS Compliant",null,10,"$0.12","$1.20"]
["660-MF1/4DCT52R2001F","MF1/4DCT52R2001F","KOA Speer",null,"Metal Film Resistors - Through Hole 1/4W 2K ohm 1% 2K OHM 1%","RoHS Compliant",null,5,"$0.12","$0.60"]
["660-MF1/4DCT52R1242F","MF1/4DCT52R1242F","KOA Speer",null,"Metal Film Resistors - Through Hole 1/4W 12.4K ohm 1%","RoHS Compliant",null,1,"$0.12","$0.12"]
["512-2N3906BU","2N3906BU","Fairchild Semiconductor",null,"Bipolar Transistors - BJT PNP Transistor General Purpose","RoHS Compliant",null,9,"$0.19","$1.71"]
["595-TL074CN","TL074CN","Texas Instruments",null,"Operational Amplifiers - Op Amps JFET Input Low Noise","RoHS Compliant",null,5,"$0.57","$2.85"]
["512-BS170","BS170","Fairchild Semiconductor",null,"MOSFET N-Channel MOSFET","RoHS Compliant",null,1,"$0.39","$0.39"]
["652-3362P-1-103LF","3362P-1-103LF","Bourns",null,"Trimmer Resistors - Through Hole 1/4\"SQ 10KOHMS 10% 0.5WATTS","RoHS Compliant By Exemption",null,5,"$1.02","$5.10"]
["810-FK11X5R1C156M","FK11X5R1C156M","TDK",null,"Multilayer Ceramic Capacitors MLCC - Leaded 15uF 16volts X5R +/-20%","RoHS Compliant",null,1,"$0.84","$0.84"]
["581-SR205C563KAA","SR205C563KAA","AVX",null,"Multilayer Ceramic Capacitors MLCC - Leaded 50volts 0.056uF 10% X7R","RoHS Compliant",null,1,"$0.49","$0.49"]
["660-MF1/4DCT52R6650F","MF1/4DCT52R6650F","KOA Speer",null,"Metal Film Resistors - Through Hole 1/4W 665 ohm 1%","RoHS Compliant",null,4,"$0.12","$0.48"]
["660-MF1/4DCT52R1501F","MF1/4DCT52R1501F","KOA Speer",null,"Metal Film Resistors - Through Hole 1/4W 1.5K ohm 1% 1.5K OHM 1%","RoHS Compliant",null,4,"$0.12","$0.48"]
["611-7201-051","7201MD9ABE","C&K Components",null,"Toggle Switches ON-ON DPDT RA PC","RoHS Compliant",null,8,"$6.61","$52.88"]
["660-MF1/4DCT52R2321F","MF1/4DCT52R2321F","KOA Speer",null,"Metal Film Resistors - Through Hole 1/4W 2.32K ohm 1% 2.32K OHM 1%","RoHS Compliant",null,8,"$0.12","$0.96"]
["926-LM361N/NOPB","LM361N/NOPB","Texas Instruments",null,"Analog Comparators Hi Speed Diff Cmptr","RoHS Compliant",null,4,"$2.70","$10.80"]
["660-MF1/4DCT52R2211F","MF1/4DCT52R2211F","KOA Speer",null,"Metal Film Resistors - Through Hole 1/4W 2.21K ohm 1% 2.21K OHM 1%","RoHS Compliant",null,4,"$0.12","$0.48"]
["660-MF1/4DCT52R1652F","MF1/4DCT52R1652F","KOA Speer",null,"Metal Film Resistors - Through Hole 1/4 WATT 16.5K OHM 1%","RoHS Compliant",null,8,"$0.12","$0.96"]
["660-MF1/4DCT52R4021F","MF1/4DCT52R4021F2","KOA Speer",null,"Metal Film Resistors - Through Hole 4.02Kohms 1% 100PPM","RoHS Compliant",null,12,"$0.12","$1.44"]
["660-MF1/4DCT52R8251F","MF1/4DCT52R8251F","KOA Speer",null,"Metal Film Resistors - Through Hole 1/4W 8.25K ohm 1%","RoHS Compliant",null,4,"$0.12","$0.48"]
["660-MF1/4DCT52R1204F","MF1/4DCT52R1204F","KOA Speer",null,"Metal Film Resistors - Through Hole 1/4 WATT 1.2M OHM 1%","RoHS Compliant",null,4,"$0.12","$0.48"]
["660-MF1/4DCT52R2051F","MF1/4DCT52R2051F","KOA Speer",null,"Metal Film Resistors - Through Hole 1/4W 2.05K ohm 1%","RoHS Compliant",null,4,"$0.12","$0.48"]
["594-K101J15C0GF53L2","K101J15C0GF53L2","Vishay",null,"Multilayer Ceramic Capacitors MLCC - Leaded 100pF 50volts 5% .1LS C0G/NPO","RoHS Compliant By Exemption",null,4,"$0.10","$0.40"]
["594-K151J15C0GF53L2","K151J15C0GF53L2","Vishay",null,"Multilayer Ceramic Capacitors MLCC - Leaded 150pF 50volts 5% C0G 2.5mm LS","RoHS Compliant By Exemption",null,4,"$0.38","$1.52"]
["810-FK16C0G1H473J","FK16C0G1H473J","TDK",null,"Multilayer Ceramic Capacitors MLCC - Leaded 0.047uF 50volts C0G +/-5%","RoHS Compliant",null,4,"$0.63","$2.52"]
["810-FG18C0G1H150JNT0","FG18C0G1H150JNT00","TDK",null,"Multilayer Ceramic Capacitors MLCC - Leaded 15pF 50volts C0G 5% Radial LS:2.5mm","RoHS Compliant","New Product",4,"$0.16","$0.64"]
["810-FG18X5R1H105KRT0","FG18X5R1H105KRT00","TDK",null,"Multilayer Ceramic Capacitors MLCC - Leaded 1uF 50volts X5R 10% Radial LS:2.5mm","RoHS Compliant","New Product",4,"$0.28","$1.12"]
["595-CD4066BE","CD4066BE","Texas Instruments",null,"Analog Switch ICs Quad","RoHS Compliant",null,4,"$0.47","$1.88"]

{"sheet":"Cadet 21 BOM","index":10,"n_rows":103,"n_cols":13,"rows_kept":103,"cut":false,"hidden":false,"merged":[]}
["Line Item","Quantity","Reference Designators","Manufacturer","Manufacturer P/N","Vendor","Vendor P/N","Description","Value","Package","Part Type","Assembly Location","Notes"]
[1,1,"-","LZX Industries","LZX-C1-PCB","LZX Industries","LZX-C1-PCB","LZX Industries Cadet I Sync Generator PCB","-","-","Fabricated","-"]
[2,1,"-","LZX Industries","LZX-C2-PCB","LZX Industries","LZX-C2-PCB","LZX Industries Cadet II RGB Encoder PCB","-","-","Fabricated","-"]
[3,1,"-","LZX Industries","LZX-C3-PCB","LZX Industries","LZX-C3-PCB","LZX Industries Cadet III Video Input PCB","-","-","Fabricated","-"]
[4,1,"-","LZX Industries","LZX-C4-PCB","LZX Industries","LZX-C4-PCB","LZX Industries Cadet IV Ramp Generator PCB","-","-","Fabricated","-"]
[5,1,"-","LZX Industries","LZX-C5-PCB","LZX Industries","LZX-C5-PCB","LZX Industries Cadet V Scaler PCB","-","-","Fabricated","-"]
[6,4,"-","LZX Industries","LZX-C6-PCB","LZX Industries","LZX-C6-PCB","LZX Industries Cadet VI Fader PCB","-","-","Fabricated","-"]
[7,4,"-","LZX Industries","LZX-C7-PCB","LZX Industries","LZX-C7-PCB","LZX Industries Cadet VII Processor PCB","-","-","Fabricated","-"]
[8,4,"-","LZX Industries","LZX-C8-PCB","LZX Industries","LZX-C8-PCB","LZX Industries Cadet VIII Hard Synch Generator PCB","-","-","Fabricated","-"]
[9,4,"-","LZX Industries","LZX-C9-PCB","LZX Industries","LZX-C9-PCB","LZX Industries Cadet IX VCO PCB","-","-","Fabricated","-"]
[10,1,"-","LZX Industries","LZX-C1-FPN","LZX Industries","LZX-C1-FPN","LZX Industries Cadet I Sync Generator Frontpanel","-","-","Fabricated","-"]
[11,1,"-","LZX Industries","LZX-C2-FPN","LZX Industries","LZX-C2-FPN","LZX Industries Cadet II RGB Encoder Frontpanel","-","-","Fabricated","-"]
[12,1,"-","LZX Industries","LZX-C3-FPN","LZX Industries","LZX-C3-FPN","LZX Industries Cadet III Video Input Frontpanel","-","-","Fabricated","-"]
[13,1,"-","LZX Industries","LZX-C4-FPN","LZX Industries","LZX-C4-FPN","LZX Industries Cadet IV Ramp Generator Frontpanel","-","-","Fabricated","-"]
[14,1,"-","LZX Industries","LZX-C5-FPN","LZX Industries","LZX-C5-FPN","LZX Industries Cadet V Scaler Frontpanel","-","-","Fabricated","-"]
[15,4,"-","LZX Industries","LZX-C6-FPN","LZX Industries","LZX-C6-FPN","LZX Industries Cadet VI Fader Frontpanel","-","-","Fabricated","-"]
[16,4,"-","LZX Industries","LZX-C7-FPN","LZX Industries","LZX-C7-FPN","LZX Industries Cadet VII Processor Frontpanel","-","-","Fabricated","-"]
[17,4,"-","LZX Industries","LZX-C8-FPN","LZX Industries","LZX-C8-FPN","LZX Industries Cadet VIII Hard Key Generator Frontpanel","-","-","Fabricated","-"]
[18,4,"-","LZX Industries","LZX-C9-FPN","LZX Industries","LZX-C9-FPN","LZX Industries Cadet IX VCO Frontpanel","-","-","Fabricated","-"]
[19,12,"[C1(I,II,III,IV,VIII)],[C3,C4,C7,C8(V)],[C3(IX)]","Vishay / Sprague","1C10Z5U334M050B ","Mouser","75-1C10Z5U334M050B ","Multilayer Ceramic Capacitors MLCC - Leaded 0.33uF 50volts Z5U 20% 2.5mm L/S","330 n","-","Through Hole","I,II,III,IV,(4)VIII,(4)IX"]
[20,184,"[C3, C4, C5, C7, C8, C9, C10, C11, C13, C14, C15, C16, C22(I)],[C3, C4, C5, C7, C8, C10, C12, C13, C14, C15, C16, C22, C23, C24, C25, C26, C27(II)],[C3, C4, C5, C7, C8, C9, C10, C11, C12, C13, C14, C16, C20, C22(III)],[C3, C4, C7, C8, C9, C10, C12, C15, C16, C17, C22, C25(IV)],[C3, C4, C7, C8(V)],[C3, C4, C5, C7, C8, C9(VI)],[C3, C4, C5, C7, C8, C9(VII)],[C3, C4, C5, C7, C8, C9, C10, C12, C13, C22(VIII)],[C9, C14, C15, C24, C25, C26, C27, C28, C29, C30, C54(IX)]","Vishay / Sprague","1C10Z5U104M050B","Mouser","75-1C10Z5U104M050B","Multilayer Ceramic Capacitors MLCC - Leaded 0.1uF 50volts Z5U 20% 2.5mm L/S","0.1 u","-","Through Hole","(13)I,(17)II,(14)III,(4)IV,(4)V,(24)VI,(24)VII,(40)VIII,(44)IX"]
[21,42,"[C2, C6(I,II,III,IV,V,VI,VII,VIII)],[C4, C8(IX)]","Panasonic","ECE-A1VKS100","Mouser","667-ECE-A1VKS100","Aluminum Electrolytic Capacitors - Leaded 10UF 35V KS RADIAL","10 u","-","Through Hole","(2)I,(2)II,(2)III,(2)IV,(2)V,(8)VI,(8)VII(8)VIII,(8)IX"]
[22,2,"[C17, C19(I)]","Vishay / BC Components","K102K15X7RH53L2","Mouser","594-K102K15X7RH53L2","Multilayer Ceramic Capacitors MLCC - Leaded 1000pF 100volts 10% X7R 2.5mm LS","1000 p","-","Through Hole","(2)I"]
[23,1,"[C18(I)]","Xicon","21RD747-RC","Mouser","21RD747-RC","Multilayer Ceramic Capacitors MLCC - Leaded 47pF 50volts C0G 5% 2.5mm L/S","47 p","-","Through Hole","(1)I"]
[24,2,"[C9, C11(II)]","TDK","FG18X7R1E105KRT06","Mouser","810-FG18X7R1E105KRT6","Multilayer Ceramic Capacitors MLCC - Leaded 1uF 25volts X7R +/-10% LS=2.5mm","1 u","-","Through Hole","(2)II"]
[25,2,"[C18, C19(II)]","Panasonic","ECA-0JM221","Mouser","667-ECA-0JM221","Aluminum Electrolytic Capacitors - Leaded 220UF 6.3V ALUM LYTIC RADIAL","220 u","-","Through Hole","(2)II"]
[26,2,"[C20, C21(II)]","AVX","TAP106K025SCS","Mouser","581-TAP106K025SCS","Tantalum Capacitors - Solid Leaded 25volts 10uF 10%","10 u","-","Through Hole","(2)II"]
[27,1,"C18(IV)]","TDK","FK11X5R1C156M","Mouser","810-FK11X5R1C156M","Multilayer Ceramic Capacitors MLCC - Leaded 15uF 16volts X5R +/-20%","15 u","-","Through Hole","(1)IV"]
[28,1,"[C29(IV)]","AVX","SR205C563KAA","Mouser","581-SR205C563KAA",null,"56 n","-","Through Hole","(1)IV"]
[29,4,"[C13(IX)]","Vishay / BC Components","K101J15C0GF53L2","Mouser","594-K101J15C0GF53L2","Multilayer Ceramic Capacitors MLCC - Leaded 100pF 50volts 5% .1LS C0G/NPO","100p","-","Through Hole","(4)IX"]
[30,4,"[C16(IX)]","Vishay / BC Components","K151J15C0GF53L2","Mouser","594-K151J15C0GF53L2","Multilayer Ceramic Capacitors MLCC - Leaded 100pF 50volts 5% .1LS C0G/NPO","150p","-","Through Hole","(4)IX"]
[31,4,"[C17(IX)]","TDK","FK16C0G1H473J","Mouser","810-FK16C0G1H473J","Multilayer Ceramic Capacitors MLCC - Leaded 0.047uF 50volts C0G +/-5%","47nF","-","Through Hole","(4)IX"]
[32,4,"[C18(IX)]","TDK","FG18C0G1H150JNT00","Mouser","810-FG18C0G1H150JNT0","Multilayer Ceramic Capacitors MLCC - Leaded 15pF 50volts C0G 5% Radial LS:2.5mm","15pF","-","Through Hole","(4)IX"]
[33,4,"[C22(IX)]","TDK","FG18X5R1H105KRT00","Mouser","810-FG18X5R1H105KRT0","Multilayer Ceramic Capacitors MLCC - Leaded 1uF 50volts X5R 10% Radial LS:2.5mm","1uF","-","Through Hole","(4)IX"]
[34,4,"[C23(IX)]","Vishay / BC Components","K102K15X7RH53L2","Mouser","594-K102K15X7RH53L2","Multilayer Ceramic Capacitors MLCC - Leaded 1000pF 100volts 10% X7R 2.5mm LS","1000 p","-","Through Hole","(4)IX"]
[35,42,"[D1, D2(I,II,III,IV,V,VI,VII,VIII)],[D7, D8(IX)]","Fairchild Semiconductor","1N4001","Mouser","512-1N4001","Rectifiers Vr/50V Io/1A T/R","-","-","Through Hole","(2)I,(2)II,(2)III,(2)IV,(2)V,(8)VI,(8)VII,(8)VIII,(8)IX","N/A on Mouser/Obsolete"]
[36,10,"[D3, D4(II)],[D4, D6(IX)]","Fairchild Semiconductor","1N4148","Mouser","512-1N4148","Diodes - General Purpose, Power, Switching 100V Io/200mA BULK","-","DO35","Through Hole","(2)II,(8)IX"]
[37,18,"[D5, D6, D7, D8, D9, D10, D11, D12, D13, D14, D15, D16(II)],[D5, D6(III)],[D3, D4, D5, D6(IV)]","STMicroelectronics","1N5711","Mouser","511-1N5711","Schottky Diodes & Rectifiers 15mA 70 Volt","-","DO35","Through Hole","(12)II,(2)III,(4)IV,"]
[38,94,"[R2, R5, R16, R17, R20, R23(I)],[R1, R2, R6(II)],[R16(III)],[R8, R12, R13, R15, R18, R31, R32, R33, R49, R50(IV)],[R2, R5, R16, R19(V)],[R1, R5, R12, R19(VI)],[R1, R12, R19(VII)],[R1, R12, R16, R25(VIII)],[R1, R10, R11, R145, R150(IX)]","KOA Speer","MF1/4DCT52R4990F","Mouser","660-MF1/4DCT52R4990F","Metal Film Resistors - Through Hole 1/4W 499 ohm 1% 500 OHM 1%","499R","-","Through Hole","(6)I,(3)II,(1)III,(16)IV,(4)V,(16)VI,(12)VII,(16)VIII,(20)IX"]
[39,13,"[R10(I)],[R13, R23(VIII)],[R107(IX)]","KOA Speer","MF1/4DCT52R4992F","Mouser","660-MF1/4DCT52R4992F","Metal Film Resistors - Through Hole 1/4W 49.9K ohm 1% 500 OHM 1%","49.9K","-","Through Hole","(1)I,(8)VIII,(4)IX"]
[40,3,"[R1, R3, R15(I)]","KOA Speer","MF1/4DCT52R3921F","Mouser","660-MF1/4DCT52R3921F","Metal Film Resistors - Through Hole 1/4W 3.92K ohm 1% 4.99K OHM 1%","3.92K","-","Through Hole","(3)I"]
[41,2,"[R9(I,III)]","KOA Speer","MF1/4DCT52R6803F","Mouser","660-MF1/4DCT52R6803F","Metal Film Resistors - Through Hole 680Kohms 1% 100PPM","680K","-","Through Hole","(1)I,(1)III"]
[42,155,"[R4, R6, R11, R12, R14, R18, R26, R28(I)],[R5, R10, R11, R12, R15, R16, R17, R18, R20, R21, R22, R24, R25, R26, R27, R28, R29, R30, R31, R33, R34, R35, R36, R37, R41(II)],[R4, R5, R7, R10, R17, R18, R20, R21(III)],[R7(VI)],[R5, R6, R9, R10, R14, R16, R20, R24, R26, R43(IV)],[R2, R5, R6, R7, R10, R11, R13, R15, R16(VII)],[R5, R7, R15, R17, R24(VIII)],[R7, R9, R23, R27, R32, R104, R111, R112, R146, R166(IX)]","KOA Speer","MF1/4DCT52R1001F","Mouser","660-MF1/4DCT52R1001F","Metal Film Resistors - Through Hole 1Kohms 1% 100PPM","1K","-","Through Hole","(8)I,(25)II,(8)III,(10)IV,(8)VI,(36)VII,(20)VIII,(40)IX"]
[43,14,"[R8, R9(I)],[R7, R19(II)],[R8, R19(III)],[R42, R113(IX)]","KOA Speer","MF1/4DCT52R75R0F","Mouser","660-MF1/4DCT52R75R0F","Metal Film Resistors – Through Hole 1/4W 75 ohm 1% ","75R","-","Through Hole","(2)I,(2)II,(2)III,(8)IX"]
[44,59,"[R7, R21, R22, R24(I)],[R8, R9(II)],[R2, R13, R15, R24(III)],[R22, R23, R28, R29, R39, R41, R42, R46, R47(IV)],[R8, R9, R11, R21, R22(VI)],[R8, R9(VII)],[R21, R27(VIII)],[R5(IX)]","KOA Speer","MF1/4DCT52R1002F","Mouser","660-MF1/4DCT52R1002F","Metal Film Resistors - Through Hole 10Kohms 1% 100PPM","10K","-","Through Hole","(4)I,(2)II,(4)III,(9)IV,(20)VI,(8)VII,(8)VIII,(4)IX"]
[45,1,"[R13(I)]","TE Connectivity / Holsworthy","1623934-1","Mouser","279-1623934-1","Metal Film Resistors - Through Hole 0Ohm 1/4W LINK","0R","-","Through Hole","(1)I"]
[46,71,"[R38(II)],[R22(III)],[R2, R4, R25, R38, R44(IV)],[R4, R6, R12, R14, R18, R20, R26, R28(V)],[R2, R18(VI)],[R18, R21(VII)],[R2, R8, R9, R11, R18, R22, R26(VIII)],[R18, R147, R148(IX)]","KOA Speer","MF1/4DCT52R4991F","Mouser","660-MF1/4DCT52R4991F","Metal Film Resistors - Through Hole 1/4W 4.99K ohm 1% 500 OHM 1%","4.99K","-","Through Hole","(1)II,(1)III,(5)IV,(8)V,(8)VI,(8)VII,(28)VIII,(12)IX"]
[47,4,"[R13, R23, R32(II)],[R6(III)]","KOA Speer","MF1/4DCT52R1401F","Mouser","660-MF1/4DCT52R1401F","Metal Film Resistors - Through Hole 1/4W 1.4K ohm 1% ","1.4K","- ","Through Hole","(3)II,(1)III"]
[48,1,"[R40(II)]","KOA Speer","MF1/4DCT52R3481F","Mouser","660-MF1/4DCT52R3481F","Metal Film Resistors - Through Hole 1/4W 3.48K ohm 1% ","3.48K","-","Through Hole","(1)II"]
[49,41,"[R3, R4, R14(II)],[R1, R3(III)],[R3, R6, R14(VI)],[R3, R14(VII)],[R3, R10, R14(VIII)],[R144(IX)]","KOA Speer","MF1/4DCT52R1003F","Mouser","660-MF1/4DCT52R1003F","Metal Film Resistors - Through Hole 100Kohms 1% 100PPM","100K","-","Through Hole","(3)II,(2)III,(12)VI,(8)VII,(12)VIII,(4)IX"]
[50,1,"[R11(III)]","KOA Speer","MF1/4DCT52R2491F","Mouser","660-MF1/4DCT52R2491F","Metal Film Resistors - Through Hole 2.49Kohms 1% 100PPM","2.49K","-","Through Hole","(1)III"]
[51,1,"[R23(III)]","KOA Speer","MF1/4DCT52R1502F","Mouser","660-MF1/4DCT52R1502F","Metal Film Resistors - Through Hole 15Kohms 1% 100PPM","15K","-","Through Hole","(1)III"]
[52,6,"Resistor","KOA Speer","MF1/4DCT52R1000F","Mouser","660-MF1/4DCT52R1000F","Metal Film Resistors - Through Hole 100 ohms 1% 100PPM","100R","-","Through Hole","(2)IV,(4)IX"]
[53,10,"Resistor","KOA Speer","MF1/4DCT52R2002F","Mouser","660-MF1/4DCT52R2002F","Metal Film Resistors - Through Hole 20Kohms 1% 100PPM","20K","-","Through Hole","(2)IV,(4)V,(4)VII"]
[54,6,"Resistor","KOA Speer","MF1/4DCT52R2001F","Mouser","660-MF1/4DCT52R2001F","Metal Film Resistors - Through Hole 2Kohms 1% 100PPM","2K","-","Through Hole","(2)IV,(4)IX"]
[55,1,"Resistor","KOA Speer","MF1/4DCT52R1242F","Mouser","660-MF1/4DCT52R1242F","Metal Film Resistors - Through Hole 10Kohms 1% 100PPM","12.4K","-","Through Hole","(1)IV,"]
[56,6,"Resistor","Bourns","3362P-1-103LF","Mouser","652-3362P-1-103LF","Trimmer Resistors - Through Hole 1/4\"SQ 10KOHMS 10% 0.5WATTS","10K","-","Through Hole","(2)IV,(4)IX"]
[57,8,"Resistor","KOA Speer","MF1/4DCT52R6650F","Mouser","660-MF1/4DCT52R6650F","Metal Film Resistors – Through Hole 1/4W 665 ohm 1% ","665R","-","Through Hole","(8)VI"]
[58,8,"Resistor","KOA Speer","MF1/4DCT52R1501F","Mouser","660-MF1/4DCT52R1501F","Metal Film Resistors - Through Hole 1/4W 1.5K ohm 1% 1.5K OHM 1%","1.5K","-","Through Hole","(8)VI"]
[59,8,"Resistor","KOA Speer","MF1/4DCT52R2321F","Mouser","660-MF1/4DCT52R2321F","Metal Film Resistors - Through Hole 2.32Kohms 1% 100PPM","2.32K","-","Through Hole","(8)VIII"]
[60,4,"R164","KOA Speer","MF1/4DCT52R2211F","Mouser","660-MF1/4DCT52R2211F","Metal Film Resistors - Through Hole 2.21Kohms 1% 100PPM","2.21K","-","Through Hole","(4)IX"]
[61,8,"R2, R30","KOA Speer","MF1/4DCT52R1652F","Mouser","660-MF1/4DCT52R1652F","Metal Film Resistors - Through Hole 16.5Kohms 1% 100PPM","16.5K","-","Through Hole","(8)IX"]
[62,12,"R3, R8, R25","KOA Speer","MF1/4DCT52R4021F","Mouser","660-MF1/4DCT52R4021F","Metal Film Resistors - Through Hole 4.02Kohms 1% 100PPM","4.02K","-","Through Hole","(12)IX"]
[63,4,"R46","KOA Speer","MF1/4DCT52R8251F","Mouser","660-MF1/4DCT52R8251F","Metal Film Resistors - Through Hole 8.25Kohms 1% 100PPM","8.25K","-","Through Hole","(4)IX"]
[64,4,"R47","KOA Speer","MF1/4DCT52R1204F","Mouser","660-MF1/4DCT52R1204F","Metal Film Resistors - Through Hole 1.2M ohms 1% 100PPM","1.2M","-","Through Hole","(4)IX"]
[65,4,"R106","KOA Speer","MF1/4DCT52R2051F","Mouser","660-MF1/4DCT52R2051F","Metal Film Resistors - Through Hole 2.05Kohms 1% 100PPM","2.05K","-","Through Hole","(4)IX"]
[66,46,"F","Fair-Rite",2743001111,"Mouser","623-2743001111","EMI Filter Beads, Chips & Arrays 43 BEAD ON LEAD Z=68 OHM @ 100MHz","-","-","Through Hole","(2)I,(2)II,(2)III,(2)IV,(2)V,(8)VI,(8)VII,(8)VIII,(12)IX"]
[67,41,"U1, U2","Texas Instruments","LM6172IN/NOPB","Mouser","926-LM6172IN/NOPB","Operational Amplifiers - Op Amps Dual High Speed,Low Pwr Amp","-","DIP8","Through Hole","(2)I,(5)II,(2)III,(2)IV,(2)V,(4)VI,(8)VII,(8)VIII,(8)IX"]
[68,12,"U3","STMicroelectronics","L7805CV","Mouser","511-L7805CV","Linear Voltage Regulators 5.0V 1.0A Positive ","-","TO220","Through Hole","(1)I,(1)II,(1)III,(1)IV,(4)VIII,(4)IX"]
[69,1,"U5","Atmel","ATMEGA88A-PU","Mouser","556-ATMEGA88A-PU","8-bit Microcontrollers - MCU AVR 8KB FLSH 512B EE 1KB SRAM-20MHz","-","DIP28","Through Hole","(1)I"]
[70,2,"U6","Texas Instruments","LM1881N/NOPB","Mouser","926-LM1881N/NOPB","Video ICs Video Sync Separator","-","DIP8","Through Hole","(1)I,(1)III"]
[71,7,"U7","Texas Instruments","SN74HC14N","Mouser","595-SN74HC14N","Inverters Hex Schmitt-Trigger ","-","DIP14","Through Hole","(1)I,(1)II,(1)IV,(4)IX"]
[72,1,"U8","Texas Instruments","CD74HC4538E","Mouser","595-CD74HC4538E","Monostable Multivibrator Dual Retrig Mono ","-","DIP16","Through Hole","(1)I"]
[73,1,"U9","Texas Instruments","CD74HC4046AE","Mouser","595-CD74HC4046AE","Phase Locked Loops - PLL PLL w/ VCO","-","DIP16","Through Hole","(1)I"]
[74,1,"U4","Analog Devices","AD724JRZ","Mouser","584-AD724JRZ","Video ICs RGB-NTSC/PAL ENCODER","-","SOIC16","SMT","(1)II"]
[75,2,"U5","Texas Instruments","CD4053BE","Mouser","595-CD4053BE","Multiplexer Switch ICs Triple 2-Ch Analog","-","DIP16","Through Hole","(1)II,(1)III,"]
[76,21,"U11","Texas Instruments","TL431BQLPR","Mouser","595-TL431BQLPR","Voltage References Adjustable Precision Shunt Regulator","-","TO-92-3","Through Hole","(1)II,(1)III,(3)IV,(4)VI,(4)VII,(4)VIII,(4)IX"]
[77,18,"U10","Texas Instruments","TL072IP","Mouser","595-TL072IP","Operational Amplifiers - Op Amps Dual JFET In Low N","-","DIP8","Through Hole","(1)III,(1)IV,(4)VI,(4)VIII,(8)IX"]
[78,3,"U12, U13","Texas Instruments","TL074CN","Mouser","595-TL074CN","Operational Amplifiers - Op Amps JFET Input Low Noise","-","DIP14","Through Hole","(2)IV,(1)VII"]
[79,4,"U2","Texas Instruments","LM361N/NOPB","Mouser","926-LM361N/NOPB","Analog Comparators Hi Speed Diff Cmptr","-","DIP14","Through Hole","(4)VIII"]
[80,4,"U11","Texas Instruments","CD4066BE","Mouser","595-CD4066BE","Analog Switch ICs Quad","-","DIP-14","Through Hole","(4)IX"]
[81,6,"J3, J5","CUI","RCJ-044","Mouser","490-RCJ-044 ","RCA Phono Connectors, Right Angle, Yellow","-","-","Through Hole","(2)I,(2)II,(2)III"]
[82,3,"M1","Keystone",621,"Mouser","534-621","Mounting Hardware THRD BRKT STL Z PL","-","-","Mechanical","(1)I,(1)II,(1)III"]
[83,1,"Y1","ABRACON","ABL-3.579545MHZ-B2","Mouser","815-ABL-3.579545B2","Crystals +/-20ppm 3.579545MHZ FUNDAMENTAL","-","HC49","Through Hole","(1)II"]
[84,1,"Y2","ECS","ECS-44-20-4X","Mouser","520-HCU443-20X","Crystals 4.433618MHz 20pF","-","HC49","Through Hole","(1)II"]
[85,17,"Q1 , Q2A*, Q2B*, Q4A*, Q4B*","Fairchild Semiconductor","2N3904BU","Mouser","512-2N3904BU ","Bipolar Transistors - BJT NPN Transistor General Purpose ","-","TO-92-3","Through Hole","(1)III,(16)IX*"]
[86,10,"Q5A*, Q5B*","Fairchild Semiconductor","2N3906BU","Mouser","512-2N3906BU","Bipolar Transistors - BJT PNP Transistor General Purpose","-","TO-92-3","Through Hole","(2)IV,(8)IX*"]
[87,2,"Q3, Q4","Fairchild Semiconductor","BS170","Mouser","512-BS170","MOSFET N-Channel MOSFET","-","TO-92-3","Through Hole","(2)IV"]
[88,4,"S1","C&K Components","7201MD9ABE","Mouser","611-7201-051","Toggle Switches ON-ON DPDT RA PC","-","-","Through Hole","(4)VII"]
[89,6,"S1","Mountain Switch","10TF230","Mouser","10TF230","Toggle Switches SPDT ON-ON RT ANGLE ","-","-","Through Hole","(1)I,(1)II,(4)IX","Only available in orders of 100 + on Mouser"]
[90,4,"S1","C&K Components","7201MD9ABE","Mouser","611-7201-051","Toggle Switches ON-ON DPDT RA PC","-","-","Through Hole","(4)IX"]
[91,4,"U2","Linear Technology","LT1251CN#PBF","Linear Technology","LT1251CN#PBF","40MHz Video Fader and DC Gain Controlled Amplifier","-","DIP16","Through Hole","(4)VI"]
[92,1,"X1","Citizen Finedevice Co Ltd","CSX750VCB13.500M-UT","DigiKey","300-8162-1-ND","OSC VCXO 13.5MHZ CMOS SMD","-","-","SMT","(1)I"]
[93,5,"-","-","-","McMaster-Carr","90272A106","Zinc-Plated Steel Pan Head Phillips Machine Screw, 4-40 Thread, 1/4\" Length","-","-","Mechanical","(2)I,(1)II,(2)III"]
[94,73,"J2, J4, J6","Wenzhou QingPu","PJ302M","Thonk","MECH_JK_PJ302M","Right angled 3.5mm Jack Sockets w/Knurled Nuts, No Washers","-","-","Through Hole","(3)I,(3)II,(1)III,(8)V,(6)IV,(16)VI,(12)VII,(16)VIII,(8)IX"]
[95,34,"R12, R14","-","-","Thonk","Mech_Pot_Alpha","Right Angle B10K Alpha 9mm Potentiometer","B10K","-","Through Hole","(2)III,(8)VI,(8)VII,(8)VIII,(8)IX"]
[96,34,"-","-","-","Thonk","Davies_1900h","Davies 1900H Clone Red (6.35mm Round Shaft)","-","-","Control Knobs","(2)III,(8)VI,(8)VII,(8)VIII,(8)IX"]
[97,9,"-","-","-","Thonk","Knurled Nuts","Knurled Nuts for PJ302M Jacks","-","-","Mechanical","(1)III,(8)IX"]
[98,21,"J9","-","-","Futurlec","IDCMH16 ","16 Pin Shrouded Male Headers IDC","-","-","Through Hole","(1)I,(1)II,(1)III,(1)IV,(1)V,(4)VI,(4)VII,(4)VIII,(4)IX"]
[99,7,"J1","-","-","Futurlec","IDCMH14","14 Pin Shrouded Male Headers IDC","-","-","Through Hole","(1)I,(1)II,(1)IV,(4)IX"]
[100,1,"J10","-","-","Futurlec","HEADD6","6 Pin .100\" St. Male Double Headers","-","-","Through Hole","(1)I"]
[101,21,"-","-","-","Erthenvar","Ribbon Cable - 16 to 16 ","16 Pin IDC EuroRack Power Cable","-","-","Accessories","(1)I,(1)II,(1)III,(1)IV,(1)V,(4)VI,(4)VII,(4)VIII,(4)IX"]
[102]